{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":12,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FHQ100CAVEB / RZQG71L8Y1B","FHQ71CAVEB / RZQG71L8Y1B","FHQ100CAVEB / RZQG100L8Y1B","FHQ140CAVEB / RZQG100L8Y1B","FHQ125CAVEB / RZQG125L8Y1B","FHQ140CAVEB / RZQG125L8Y1B","FHQ140CAVEB / RZQG140L7Y1B","FHQ71CAVEB / FHQ71CAVEB / RZQG125L8Y1B (Archived)"]
["Chladicí výkon","Jm.","","kW","","6.8","9.5","","12.0","","13.4"]
["Prostorové chlazení","SEER","","","6.95","6.95","6.11","6.11","6.01","6.01"]
["","Roční spotřeba energie","","kWh/a","343","343","545","545","699","699"]
["","Kapacita","Pnávrh","kW","6.80","6.8","9.5","9.50","12","12.00"]
["","Třída energetické úspornosti","","","A++","A++","A++","A++","A+","A+"]
["Prostorové vytápění (průměrné klima)","Výkon","Pnávrh","kW","7.60","7.6","11.3","11.30","14.13","14.13"]
["","SCOP/A","","","4.32","4.32","4.61","4.61","4.23","4.23"]
["","Třída energetické účinnosti","","","A+","A+","A++","A++","A+","A+"]
["","Roční spotřeba energie","","kWh/a","2,463","2,463","3,432","3,432","4,677","4,677"]
["Jmenovitá účinnost","Roční spotřeba energie","","kWh","","890","1,245","","1,790"]
["","EER","","","","3.82","3.81","","3.35","","3.31"]
["","COP","","","","4.13","4.15","","3.89","","3.63"]
["","Směrnice oenergetických štítcích","Chlazení","","","A","A","","A"]
["","","Vytápění","","","A","A","","A"]
["Topný výkon","Jm.","","kW","","7.5","10.8","","13.5","","15.5"]
["Poznámky","","","","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU"]
["","","","","","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení"]
["Outdoor unit","","","","","","","","","","","RZQG125L8Y1"]
["Prostorové chlazení","Třída energetické úspornosti","","","","","","","","","","B"]
["","Kapacita","Pnávrh","kW","","","","","","","","12.00"]
["","SEER","","","","","","","","","","5.10"]
["","Roční spotřeba energie","","kWh/a","","","","","","","","824"]
["Prostorové vytápění (průměrné klima)","Třída energetické účinnosti","","","","","","","","","","A"]
["","Výkon","Pnávrh","kW","","","","","","","","12.71"]
["","SCOP/A","","","","","","","","","","3.80"]
["","Roční spotřeba energie","","kWh/a","","","","","","","","4683"]