{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":5,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9 / RXS-L"]
[]
[]
[]
[]
["","","","","FLXS35BAVMB9 / RXS35L2V1B"]
["Chladicí výkon","Min.","","kW","1.2"]
["","Max.","","kW","3.8"]
["","Jm.","","kW","3.5"]
["Spoje potrubí","Liquid","OD","mm","6.35"]
["","Plyn","OD","mm","9.5"]
["","Drain","OD","mm","18.0"]
["Jmenovitá účinnost","Annual energy consumption","","kWh","565"]
["","EER","","","3.10"]
["","COP","","","3.57"]
["","Směrnice o energetických štítcích","Chlazení","","B"]
["","","Vytápění","","B"]
["Topný výkon","Jm.","","kW","4.0"]
["","Min.","","kW","1.4"]
["","Max.","","kW","5.0"]
["Poznámky","","","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU"]
["","","","","(2) - 220 V"]
["","","","","(3) - 230V"]
["","","","","(4) - 240 V"]
["","","","","(5) - Køling: indendørs temp: 27 °CDB, 19,0 °CWB; udendørs temp. 35°CDB, 24°CWB; tilsvarende rørlængde: 5m"]
["","","","","(6) - Vytápění: vnitřní teplota 20° CDB; vnější teplota 7° CDB, 6° CWB ekvivalentní délka potrubí chladiva: 5m"]
["","","","","(7) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení"]