{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":5,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9"]
[]
[]
[]
[]
["","","","","FLXS35BAVMB9"]
["Hladina akustického tlaku","Vytápění","Vysoké","dBA","46"]
["","","Tichý provoz","dBA","30"]
["","","Nízký","dBA","33"]
["","Chlazení","Tichý provoz","dBA","29"]
["","","Nízký","dBA","32"]
["","","Vysoké","dBA","38"]
["","","Jm.","dBA","36"]
["","Chlazení","Jm.","dBA","35"]
["Standardní příslušenství","Příručka pro instalaci","","","1"]
["","Manuální ovládání","","","1"]
["","Infračervené dálkové ovládání","","","1"]
["","Baterie AAA","","","2"]
["","Držák dálkového ovládání","","","1"]
["","Montážní deska","","","1"]
["","Tepelná izolace trubky (trubka chladiva)","","","8"]
["","Filtr pro čištění vzduchu","","","1"]
["","Fotokatalytický dezodorizační filtr","","","1"]
["","Boční kryt","","","2"]
["","Vázací páska","","","4"]
["Control systems","Infrared remote control","","","ARC433B67"]
["Připojovací rozměry","Kapalina","Vnější průměr","mm","6.35"]
["","Plyn","Vnější průměr","mm","9.5"]
["","Vypouštění","","","18"]
["Hladina akustického výkonu","Chlazení","","dBA","53"]
["","Vytápění","","dBA","59"]
["Rozměry","Jednotka","Šířka","mm","1,050"]
["","","Hloubka","mm","200"]
["","","Výška","mm","490"]
["Opláštění","Barva","","","Mandlová bílá"]
["Hmotnost","Jednotka","","kg","16"]
["Power supply","Fáze","","","1~"]
["","Frekvence","","Hz","50"]
["","Označení","","","VM"]
["","Napětí","","V","220-240"]
["Poznámky","","","","(1) - 220 V"]
["","","","","(2) - 230V"]
["","","","","(3) - 240 V"]
["","","","","(4) - Læs specifikationer til den Multi udendørs enhed, der skal tilsluttes, når den er koblet til udendørs enhed i Multi-system."]