{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":6,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNQ-A / RXS-L3"]
[]
[]
[]
[]
["","","","","FNQ25A2VEB / RXS25L3V1B","FNQ35A2VEB / RXS35L3V1B"]
["Chladicí výkon","Jm.","","kW","2.6","3.4"]
["Jmenovitá účinnost","Annual energy consumption","","kWh","345","556"]
["","EER","","","3.77 (1)","3.06 (1)"]
["","COP","","","4.00 (1)","3.48 (1)"]
["","Směrnice o energetických štítcích","Chlazení","","A","B"]
["","","Vytápění","","A","B"]
["Topný výkon","Jm.","","kW","3.20","4.00"]
["Poznámky","","","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU"]
["","","","","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení"]