{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":10,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-CB"]
[]
[]
[]
[]
["","","","","","FTXA20C2V1BB","FTXA25C2V1BB","FTXA35C2V1BB","FTXA42C2V1BB","FTXA50C2V1BB"]
["Vstup napájení","Chlazení","","Jm.","kW","0.02","0.022","0.023","0.028","0.030"]
["","Vytápění","","Jm.","kW","0.02","0.02","0.22","0.036","0.039"]
["Opláštění","Barva","","","","Černá","Černá","Černá","Černá","Černá"]
["Rozměry","Jednotka","","Výška","mm","295","295","295","295","295"]
["","","","Šířka","mm","798","798","798","798","798"]
["","","","Hloubka","mm","189","189","189","189","189"]
["Hmotnost","Jednotka","","","kg","11.5","11.5","11.5","11.5","11.5"]
["Ventilátor","Průtok vzduchu","Chlazení","Vysoké","m³/min","11","11.5","11.9","13.1","13.5"]
["","","","Střední","m³/min","8.2","8.6","8.6","9.8","10.4"]
["","","","Nízký","m³/min","6.1","6.1","6.1","7.2","7.6"]
["","","","Tichý provoz","m³/min","4.6","4.6","4.6","4.6","5.2"]
["","","Vytápění","Vysoké","m³/min","10.9","11.1","11.5","14.6","15.1"]
["","","","Střední","m³/min","8.7","9","9","10.5","11.1"]
["","","","Nízký","m³/min","6.4","6.4","6.4","7.7","8.2"]
["","","","Tichý provoz","m³/min","4.5","4.5","4.5","5.2","5.7"]
["Hladina akustického výkonu","Chlazení","","","dBA","57","57","60","60","60"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","39","40","41","45","46"]
["","","","Střední","dBA","32","33","33","37","39"]
["","","","Nízký","dBA","25","25","25","29","31"]
["","","","Tichý provoz","dBA","19","19","19","21","24"]
["","Vytápění","","Vysoké","dBA","39","40","41","45","46"]
["","","","Střední","dBA","32","33","33","37","42"]
["","","","Nízký","dBA","25","25","25","29","33"]
["","","","Tichý provoz","dBA","19","19","19","21","24"]
["Chladivo","Vliv na globální oteplování (GWP)","","","","675","675","675","675","675.0"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","6.35","6.35","6.35","6.35","6.35"]
["","Plyn","","Vnější průměr","mm","9.5","9.5","9.5","9.5","12.70"]
["","Odvod kondenzátu","","","","18","18","18","18","18"]
["Řídicí systémy","Infračervené dálkové ovládání","","","","ARC466A85","ARC466A85","ARC466A85","ARC466A85","ARC466A85"]
["","Kabelové dálkové ovládání","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Standardní příslušenství","Installation manual","","","","1","1","1","1","1"]
["","Screw cover","","","","2","2","2","2","2"]
["","AAA dry-cell batteries","","","","2","2","2","2","2"]
["","General safety precautions","","","","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1"]
["","Vzduchový filtr","","","","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1"]
["","Remote controller mounting plate","","","","1","1","1","1","1"]
["","Screw bag","","","","1","1","1","1","1"]
["Napájení","Označení","","","","V1","V1","V1","V1","V1"]
["","Fáze","","","","1~","1~","1~","1~","1~"]
["","Frekvence","","","Hz","50","50","50","50","50"]
["","Napětí","","","V","220-240","220-240","220-240","220-240","220-240"]