{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-B"]
[]
[]
[]
[]
["","","","","FTXF20B5V1B","FTXF25B5V1B"]
["Hladina akustického tlaku","Vytápění","Vysoké","dBA","39","40"]
["","","Střední","dBA","34","34"]
["","","Tichý provoz","dBA","21","21"]
["","","Nízký","dBA","28","28"]
["","Chlazení","Střední","dBA","33","33"]
["","","Tichý provoz","dBA","20","20"]
["","","Nízký","dBA","25","26"]
["","","Vysoké","dBA","39","40"]
["Standardní příslušenství","Příručka pro instalaci","","","1","1"]
["","Manuální ovládání","","","1","1"]
["","Infračervené dálkové ovládání","","","1","1"]
["","Baterie AAA","","","2","2"]
["","Držák dálkového ovládání","","","1","1"]
["","Montážní deska","","","1","1"]
["","Upevňovací šrouby vnitřní jednotky","","","2","2"]
["Řídicí systémy","Wired remote control","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["","Infrared remote control","","","ARC470A1","ARC470A1"]
["Piping connections","Kapalina","Vnější průměr","mm","6.35","6.35"]
["","Plyn","Vnější průměr","mm","9.50","9.50"]
["","Vypouštění","","","18","18"]
["Příkon","Chlazení","Jm.","kW","0.017","0.019"]
["","Vytápění","Jm.","kW","0.020","0.020"]
["Hladina akustického výkonu","Chlazení","","dBA","55","55"]
["","Vytápění","","dBA","55","55"]
["Rozměry","Jednotka","Šířka","mm","770","770"]
["","","Hloubka","mm","225","225"]
["","","Výška","mm","286","286"]
["Opláštění","Colour","","","Bílý","Bílý"]
["Hmotnost","Jednotka","","kg","8.50","8.50"]
["Power supply","Phase","","","1~","1~"]
["","Frekvence","","Hz","50","50"]
["","Napětí","","V","220-240","220-240"]