{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":8,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXG-LW / RXG-L"]
[]
[]
[]
[]
["","","","","FTXG20LV1BW / RXG20L2V1B","FTXG25LV1BW / RXG25L2V1B","FTXG35LV1BW / RXG35L2V1B","FTXG50LV1BW / RXG50L2V1B"]
["Chladicí výkon","Min.","","kW","1.3","1.3","1.4","1.7"]
["","Max.","","kW","2.8","3.0","3.8","5.3"]
["Topný výkon","Min.","","kW","1.3","1.3","1.4","1.7"]
["","Max.","","kW","4.3","4.5","5.0","6.5"]
["Jmenovitá účinnost","EER","","","4.59","4.59","3.97","3.53"]
["","COP","","","5.00","4.42","4.06","3.65"]
["","Roční spotřeba energie","","kWh","250.5","261.5","441","680"]
["","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích-=-Chlazení","","A","A","A","A"]
["","","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích-=-Vytápění","","A","A","A","A"]
["Spoje potrubí","Vypouštění","OD","mm","18","18.0","18.0","18.0"]
["Připojovací rozměry","Plyn","Vnější průměr","mm","9.5","9.5","9.5","12.7"]
["","Kapalina","Vnější průměr","mm","6.35","6.35","6.35","6.35"]
["Prostorové chlazení","Třída energetické úspornosti","","","A+++","A+++","A++","A++"]
["","Kapacita","Pnávrh","kW","2.30","2.40","3.50","4.80"]
["","SEER","","","8.52","8.50","7.00","6.70"]
["","Roční spotřeba energie","","kWh/r","94","99","175","251"]
["Prostorové vytápění (průměrné klima)","Třída energetické účinnosti","","","A++","A++","A++","A+"]
["","Výkon","Pnávrh","kW","2.10","2.70","3.00","4.60"]
["","SCOP/A","","","4.60","4.60","4.60","4.24"]
["","Roční spotřeba energie","","kWh/r","639","821","913","1519"]
["Poznámky","","","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU"]
["","","","","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení"]
["","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V"]