{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MS / 3MXM-A9"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BS / FTXJ20MV1BS / 3MXM40A2V1B9"]
["Chladicí výkon","Jm.","","kW","4.00"]
["Topný výkon","Jm.","","kW","4.60"]
["Jmenovitá účinnost","EER","","","4.15"]
["","COP","","","3.95"]
["","Roční spotřeba energie","","kWh","482"]
["","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích-=-Chlazení","","A"]
["","","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích-=-Vytápění","","A"]
["Prostorové chlazení","Třída energetické úspornosti","","","A++"]
["","Kapacita","Pnávrh","kW","4.00"]
["","SEER","","","7.62"]
["","Roční spotřeba energie","","kWh/a","164"]
["Prostorové vytápění (průměrné klima)","Třída energetické účinnosti","","","A+"]
["","Výkon","Pnávrh","kW","4.80"]
["","SCOP/A","","","4.11"]
["","Topný výkon Pdh při -10°","","kW","3.58"]
["","Roční spotřeba energie","","kWh/a","1632"]