{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MS / 4MXM-A"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 4MXM80A2V1B"]
["Chladicí výkon","Jm.","","kW","7.50"]
["Prostorové chlazení","SEER","","","6.92"]
["","Roční spotřeba energie","","kWh/rok","380"]
["","Kapacita","Pnávrh","kW","7.50"]
["","Třída energetické úspornosti","","","A++"]
["Prostorové vytápění (průměrné klima)","Výkon","Pnávrh","kW","6.46"]
["","SCOP/A","","","4.02"]
["","Třída energetické účinnosti","","","A+"]
["","Roční spotřeba energie","","kWh/rok","2,245"]
["Jmenovitá účinnost","Roční spotřeba energie","","kWh","908"]
["","EER","","","4.13"]
["","COP","","","3.32"]
["","Směrnice oenergetických štítcích","Chlazení","","A"]
["","","Vytápění","","C"]
["Topný výkon","Jm.","","kW","10.00"]
["Poznámky","","","","(1) - Jmenovité chladicí výkony vycházejí z těchto podmínek: vnitřní teplota: 27°CDB, 19°CWB, venkovní teplota: 35 °CDB, ekvivalentní délka potrubí s chladivem: 5 m, rozdíl úrovní: 0 m."]
["","","","","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]
["","","","","(3) - Viz samostatný výkres s provozním rozsahem"]
["","","","","(4) - Údaje o elektrickém systému najdete v samostatném výkresu"]