{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXL-JV / RXL-M"]
[]
[]
[]
[]
["","","","","FTXL25J2V1B / RXL25M2V1B","FTXL35J2V1B / RXL35M2V1B"]
["Chladicí výkon","Min.","","kW","1.2","1.3"]
["","Max.","","kW","3.4","3.8"]
["Spoje potrubí","Kapalina","Vnější průměr","mm","6.35","6.35"]
["","Plyn","Vnější průměr","mm","9.5","9.5"]
["","Vypouštění","OD","mm","18","18"]
["Jmenovitá účinnost","Roční spotřeba energie","","kWh","400.5","570"]
["","EER","","","3.12","3.07"]
["","COP","","","4.43","4.21"]
["","Směrnice oenergetických štítcích","Chlazení","","B","B"]
["","","Vytápění","","A","A"]
["Topný výkon","Min.","","kW","1.1","1.2"]
["","Max.","","kW","5.5","6.0"]
["Poznámky","","","","(1) - Pro minimální výkon vytápění ventilátor vnitřní jednotky nastaven na SL","(1) - Pro minimální výkon vytápění ventilátor vnitřní jednotky nastaven na SL"]
["","","","","(2) - 220 V","(2) - 220 V"]
["","","","","(3) - 230V","(3) - 230V"]
["","","","","(4) - 240 V","(4) - 240 V"]
["","","","","(5) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(5) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU"]
["","","","","(6) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","(6) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení"]