{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":6,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXLS-K3"]
[]
[]
[]
[]
["","","","","FTXLS25K3V1B","FTXLS35K3V1B"]
["Hladina akustického tlaku","Vytápění","Vysoké","dBA","47","47"]
["","","Tichý provoz","dBA","19","19"]
["","","Nízký","dBA","23","23"]
["","Chlazení","Tichý provoz","dBA","21","21"]
["","","Nízký","dBA","33","33"]
["","","Vysoké","dBA","45","45"]
["","","Jm.","dBA","37","36"]
["","Chlazení","Jm.","dBA","39","39"]
["Standardní příslušenství","Příručka pro instalaci","","","1","1"]
["","Manuální ovládání","","","1","1"]
["","Infračervené dálkové ovládání","","","1","1"]
["","Baterie","","","2","2"]
["","Držák dálkového ovládání","","","1","1"]
["","Montážní deska","","","1","1"]
["","Fotokatalytický filtr s apatitem titanu pro čištění vzduchu","","","2","2"]
["","Upevňovací šrouby vnitřní jednotky","","","2","2"]
["Řídicí systémy","Infrared remote control","","","ARC466A9","ARC466A9"]
["Připojovací rozměry","Kapalina","Vnější průměr","mm","6.35","6.35"]
["","Plyn","Vnější průměr","mm","9.5","9.5"]
["","Vypouštění","","","18","18"]
["Vstup napájení","Chlazení","Jm.","kW","0.024 (2), 0.024 (3), 0.024 (4)","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Vytápění","Jm.","kW","0.030 (2), 0.030 (3), 0.030 (4)","0.030 (2), 0.030 (3), 0.030 (4)"]
["Hladina akustického výkonu","Chlazení","","dBA","59","59"]
["","Vytápění","","dBA","62","62"]
["Rozměry","Jednotka","Šířka","mm","900","900"]
["","","Hloubka","mm","215","215"]
["","","Výška","mm","298","298"]
["Opláštění","Colour","","","Bílý","Bílý"]
["Hmotnost","Jednotka","","kg","12","12"]
["Power supply","Phase","","","1~","1~"]
["","Frekvence","","Hz","50","50"]
["","Označení","","","V1","V1"]
["","Napětí","","V","220-240","220-240"]
["Poznámky","","","","(1) - Læs specifikationer til den Multi udendørs enhed, der skal tilsluttes, når den er koblet til udendørs enhed i Multi-system.","(1) - Læs specifikationer til den Multi udendørs enhed, der skal tilsluttes, når den er koblet til udendørs enhed i Multi-system."]
["","","","","(2) - 220 V","(2) - 220 V"]
["","","","","(3) - 230V","(3) - 230V"]
["","","","","(4) - 240 V","(4) - 240 V"]