{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":16,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-A / RXM-A"]
[]
[]
[]
[]
["","","","","FTXM20A2V1B / RXM20A5V1B","FTXM20A5V1B / RXM20A5V1B","FTXM25A2V1B / RXM25A5V1B","FTXM25A5V1B / RXM25A5V1B","FTXM35A2V1B / RXM35A5V1B","FTXM35A5V1B / RXM35A5V1B","FTXM42A2V1B / RXM42A5V1B","FTXM42A5V1B / RXM42A5V1B","FTXM50A2V1B / RXM50A5V1B","FTXM50A5V1B / RXM50A5V1B","FTXM60A2V1B / RXM60A5V1B","FTXM71A2V1B / RXM71A5V1B"]
["Chladicí výkon","Min.","","kW","0.90","0.90","0.90","0.90","0.90","0.90","1.50","1.50","1.70","1.70","1.7","2.3"]
["","Jm.","","kW","2.00","2.00","2.50","2.50","3.50","3.50","4.20","4.20","5.00","5.00","6","7.1"]
["","Max.","","kW","3.00","3.00","3.80","3.80","4.40","4.40","5.20","5.20","5.30","5.30","7","8.5"]
["Topný výkon","Min.","","kW","0.80","0.80","0.80","0.80","0.80","0.80","1.50","1.50","1.70","1.70","1.7","2.3"]
["","Jm.","","kW","2.50","2.50","2.80","2.80","4.00","4.00","5.40","5.40","5.80","5.80","7","8.2"]
["","Max.","","kW","4.50","4.50","5.00","5.00","5.50","5.50","6.20","6.20","6.50","6.50","8","10.2"]
["Jmenovitá účinnost","EER","","","5.35","5.35","5.20","5.20","4.63","4.63","4.20","4.20","3.68","3.68","3.39","3.03"]
["","COP","","","5.00","5.00","5.00","5.00","4.55","4.55","4.19","4.19","4.15","4.15","3.61","3.19"]
["","Roční spotřeba energie","","kWh","187","187","240","240","378","378","500","500","679","679","885","1172"]
["","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích-=-Chlazení","","A","A","A","A","A","A","A","A","A","A","A","B"]
["","","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích-=-Vytápění","","A","A","A","A","A","A","A","A","A","A","A","D"]
["Prostorové chlazení","Třída energetické úspornosti","","","A+++","A+++","A+++","A+++","A+++","A+++","A++","A++","A++","A++","A++","A++"]
["","Kapacita","Pnávrh","kW","2.00","2.00","2.50","2.50","3.50","3.50","4.20","4.20","5.00","5.00","6","7.1"]
["","SEER","","","9.47","9.47","9.47","9.47","9.25","9.25","8.11","8.11","7.80","7.80","6.9","6.2"]
["","Roční spotřeba energie","","kWh/r","74","74","92","92","132","132","181","181","224","224","304","401"]
["Prostorové vytápění (průměrné klima)","Třída energetické účinnosti","","","A+++","A+++","A+++","A+++","A+++","A+++","A++","A++","A++","A++","A+","A+"]
["","Výkon","Pnávrh","kW","2.30","2.30","2.40","2.40","2.50","2.50","4.00","4.00","4.50","4.50","4.8","6.2"]
["","SCOP/A","","","5.20","5.20","5.20","5.20","5.20","5.20","5.00","5.00","4.80","4.80","4.3","4.1"]
["","Topný výkon Pdh při -10°","","kW","2.30","2.30","2.40","2.40","2.50","2.50","4.00","4.00","4.50","4.50","3.99","5.01"]
["","Roční spotřeba energie","","kWh/r","619","619","647","647","673","673","1120","1120","1312","1312","1,562","2116"]
["Energetickou účinná řada","","","","","","","","","","","","","","","A+++ ~ D"]