{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":5,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-R / RXM-N"]
[]
[]
[]
[]
["","","","","FTXM71R2V1B / RXM71N2V1B"]
["Chladicí výkon","Min.","","kW","2.30"]
["","Max.","","kW","8.50"]
["","Jm.","","kW","7.10"]
["Jmenovitá účinnost","Roční spotřeba energie","","kWh","1,172"]
["","EER","","","3.03"]
["","COP","","","3.19"]
["","Směrnice oenergetických štítcích","Chlazení","","B"]
["","","Vytápění","","D"]
["Topný výkon","Jm.","","kW","8.20"]
["","Min.","","kW","2.30"]
["","Max.","","kW","10.20"]
["Poznámky","","","","(1) - Viz samostatný výkres s provozním rozsahem"]
["","","","","(2) - Údaje o elektrickém systému najdete v samostatném výkresu"]
["","","","","(3) - Jmenovité chladicí výkony vycházejí z těchto podmínek: vnitřní tep.: 27°CDB, 19°CWB, venkovní teplota: 35 °CDB, ekvivalentní délka potrubí s chladivem: 5 m, rozdíl úrovní: 0 m."]
["","","","","(4) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]