{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":12,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G"]
[]
[]
[]
[]
["","","","","","FTXS20G2V1B","FTXS25G2V1B","FTXS35G2V1B","FTXS42G2V1B","FTXS50G2V1B","FTXS60GV1B","FTXS71GV1B"]
["Hladina akustického tlaku","Vytápění","","Vysoké","dBA","38","39","42","42","44","","46"]
["","","","Tichý provoz","dBA","25","25","26","30","31","","34"]
["","","","Nízký","dBA","28","28","29","33","34","","37"]
["","Chlazení","","Tichý provoz","dBA","22","22","23","30","31","","34"]
["","","","Nízký","dBA","25","25","26","33","34","","37"]
["","","","Vysoké","dBA","38","38","42","42","43","","46"]
["","","","Jm.","dBA","33","34","36","38","39","","42"]
["","Chlazení","","Jm.","dBA","32","32","34","38","39","","42"]
["Standardní příslušenství","Fotokatalytický filtr s apatitem titanu pro čištění vzduchu","","","","2","2","2","2","2"]
["","Manuální ovládání","","","","1","1","1","1","1","","1"]
["","Příručka pro instalaci","","","","1","1","1","1","1","","1"]
["","Bezdrátové dálkové ovládání","","","","1","1","1","1","1","","1"]
["","Baterie","","","","2","2","2","2","2","","2"]
["","Držák dálkového ovládání","","","","1","1","1","1","1","","1"]
["","Upevňovací šrouby vnitřní jednotky","","","","2","2","2","2","2","","2"]
["","Montážní deska","","","","1","1","1","1","1","","1"]
["Control systems","Infračervené dálkové ovládání","","","","","","","","","","ARC452A3"]
["Spoje potrubí","Kapalný","","OD","mm","6.35","6.35","6.35","6.35","6.35","","6.35"]
["","Plyn","","OD","mm","9.52","9.52","9.52","9.52","12.70","","15.9"]
["","Drain","","","","18","18","18","18","18","","18"]
["Vstup napájení","Chlazení","","Jm.","kW","","","","","","","0.045 (2), 0.045 (3), 0.045 (4)"]
["","Vytápění","","Jm.","kW","","","","","","","0.060 (2), 0.060 (3), 0.060 (4)"]
["Hladina akustického výkonu","Chlazení","","","dBA","54","54","58","58","59","","63"]
["","Vytápění","","","dBA","54","55","58","58","60","","62"]
["Rozměry","Unit","","Width","mm","800","800","800","800","800","","1,050"]
["","","","Depth","mm","215","215","215","215","215","","250"]
["","","","Height","mm","295","295","295","295","295","","290"]
["Opláštění","Barva","","","","Bílý","Bílý","Bílý","Bílý","Bílý","","Bílý"]
["Hmotnost","Unit","","","kg","9","9","10","10","10","","12"]
["Power supply","Fáze","","","","1~","1~","1~","1~","1~","","1~"]
["","Frekvence","","","Hz","50","50","50","50","50","","50"]
["","Označení","","","","V1","V1","V1","V1","V1","","V1"]
["","Napětí","","","V","220-240","220-240","220-240","220-240","220-240","","220-240"]
["Poznámky","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - SL: Luftstrømmens hastighedsindstillings lydløse ventilatorniveau"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 220 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 230V"]
["Ventilátor","Průtok vzduchu","Chlazení","Jm.","m³/min","","","","","","16.0"]
["Hladina akustického tlaku","Chlazení","","Jm.","dBA","","","","","","41"]
["Ventilátor","Průtok vzduchu","Vytápění","Jm.","m³/min","","","","","","14.9"]
["Hladina akustického tlaku","Vytápění","","Jm.","dBA","","","","","","40"]
["Vstup napájení","Chlazení","","Jm.","kW","","","","","","0.040 (4) (2) (3), 0.040 (4) (2) (3), 0.040 (4) (2) (3)"]
["","Vytápění","","Jm.","kW","","","","","","0.045 (4) (2) (3), 0.045 (4) (2) (3), 0.045 (4) (2) (3)"]
["Opláštění","Barva","","","","","","","","","Bílá"]
["Rozměry","Jednotka","","Výška","mm","","","","","","290"]
["","","","Šířka","mm","","","","","","1050"]
["","","","Hloubka","mm","","","","","","250"]
["Hmotnost","Jednotka","","","kg","","","","","","12"]
["Ventilátor","Průtok vzduchu","Chlazení","Vysoké","m³/min","","","","","","16.0"]
["","","","Nízký","m³/min","","","","","","11.3"]
["","","","Tichý provoz","m³/min","","","","","","10.1"]
["","","Vytápění","Vysoké","m³/min","","","","","","17.2"]
["","","","Nízký","m³/min","","","","","","12.6"]
["","","","Tichý provoz","m³/min","","","","","","11.3"]
["Hladina akustického výkonu","Chlazení","","","dBA","","","","","","60"]
["","Vytápění","","","dBA","","","","","","59"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","","","","","","45"]
["","","","Nízký","dBA","","","","","","36"]
["","","","Tichý provoz","dBA","","","","","","33"]
["","Vytápění","","Vysoké","dBA","","","","","","44"]
["","","","Nízký","dBA","","","","","","35"]
["","","","Tichý provoz","dBA","","","","","","32"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","","","","","","6.35"]
["","Plyn","","Vnější průměr","mm","","","","","","12.7"]
["","Odvod kondenzátu","","","","","","","","","18"]
["Řídicí systémy","Infračervené dálkové ovládání","","","","","","","","","ARC452A3"]
["Standardní příslušenství","Installation manual","","","","","","","","","1"]
["","Wireless remote control","","","","","","","","","1"]
["","Operation manual","","","","","","","","","1"]
["","Batteries","","","","","","","","","2"]
["","Indoor unit fixing screws","","","","","","","","","2"]
["","Mounting plate","","","","","","","","","1"]
["","Remote control holder","","","","","","","","","1"]
["","Titanium apatite photocatalytic air purification filter","","","","","","","","","2"]
["Napájení","Označení","","","","","","","","","V1"]
["","Fáze","","","","","","","","","1~"]
["","Frekvence","","","Hz","","","","","","50"]
["","Napětí","","","V","","","","","","220-240"]
["Standardní příslušenství","Fotokatalytický filtr s apatitem titanu pro čištění vzduchu, bez rámu","","","","","","","","","","2"]
["Poznámky","","","","","","","","","","","(4) - 240 V"]