{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":15,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K"]
[]
[]
[]
[]
["","","","","","FTXS20K2V1B","FTXS20K3V1B","FTXS25K2V1B","FTXS25K3V1B","FTXS35K2V1B","FTXS35K3V1B","FTXS42K2V1B","FTXS42K3V1B","FTXS50K2V1B","FTXS50K3V1B"]
["Hladina akustického tlaku","Vytápění","","Vysoké","dBA","40","","","","","","45"]
["","","","Tichý provoz","dBA","19","","","","","","22"]
["","","","Nízký","dBA","27","","","","","","33"]
["","Chlazení","","Tichý provoz","dBA","19","","","","","","21"]
["","","","Nízký","dBA","24","","","","","","33"]
["","","","Vysoké","dBA","40","","","","","","45"]
["","","","Jm.","dBA","34","","","","","","39"]
["","Chlazení","","Jm.","dBA","32","","","","","","39"]
["Standardní příslušenství","Příručka pro instalaci","","","","1","","","","","","1"]
["","Manuální ovládání","","","","1","","","","","","1"]
["","Bezdrátové dálkové ovládání","","","","1","","","","","","1"]
["","Baterie","","","","2","","","","","","2"]
["","Držák dálkového ovládání","","","","1","","","","","","1"]
["","Montážní deska","","","","1","","","","","","1"]
["","Upevňovací šrouby vnitřní jednotky","","","","2","","","","","","2"]
["","Fotokatalytický filtr s apatitem titanu pro čištění vzduchu","","","","2","","","","","","2"]
["Řídicí systémy","Infrared remote control","","","","ARC466A6","","","","","","ARC466A6"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","6.35","","","","","","6.35"]
["","Plyn","","Vnější průměr","mm","9.5","","","","","","9.5"]
["","Vypouštění","","","","18","","","","","","18"]
["Vstup napájení","Chlazení","","Jm.","kW","0.04","","","","","","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Vytápění","","Jm.","kW","0.04","","","","","","0.030 (2), 0.030 (3), 0.030 (4)"]
["Hladina akustického výkonu","Chlazení","","","dBA","58","","","","","","59"]
["","Vytápění","","","dBA","58","","","","","","59"]
["Rozměry","Jednotka","","Šířka","mm","780","","","","","","900"]
["","","","Hloubka","mm","215","","","","","","215"]
["","","","Výška","mm","289","","","","","","298"]
["Opláštění","Barva","","","","Bílý","","","","","","Bílý"]
["Hmotnost","Jednotka","","","kg","8","","","","","","11"]
["Power supply","Fáze","","","","1~","","","","","","1~"]
["","Frekvence","","","Hz","50","","","","","","50"]
["","Označení","","","","V1","","","","","","V1"]
["","Napětí","","","V","220-240","","","","","","220-240"]
["Poznámky","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - Læs specifikationer til den Multi udendørs enhed, der skal tilsluttes, når den er koblet til udendørs enhed i Multi-system.","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 220 V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 230V","(3) - 240 V","(3) - 240 V","(3) - 240 V"]
["Vstup napájení","Chlazení","","Jm.","kW","","0.040, 0.040, 0.040","0.04","0.040 (3) (1) (2), 0.040 (3) (1) (2), 0.040 (3) (1) (2)","0.026 (3) (4) (2), 0.026 (3) (4) (2), 0.026 (3) (4) (2)","0.026 (1) (3) (2), 0.026 (1) (3) (2), 0.026 (1) (3) (2)","","0.024, 0.024, 0.024","0.026 (4) (2) (3), 0.026 (4) (2) (3), 0.026 (4) (2) (3)","0.026 (1) (2) (3), 0.026 (1) (2) (3), 0.026 (1) (2) (3)"]
["","Vytápění","","Jm.","kW","","0.040, 0.040, 0.040","0.04","0.040 (2) (3) (1), 0.040 (2) (3) (1), 0.040 (2) (3) (1)","0.028 (2) (4) (3), 0.028 (2) (4) (3), 0.028 (2) (4) (3)","0.028 (1) (3) (2), 0.028 (1) (3) (2), 0.028 (1) (3) (2)","","0.030, 0.030, 0.030","0.032 (2) (4) (3), 0.032 (2) (4) (3), 0.032 (2) (4) (3)","0.032 (2) (1) (3), 0.032 (2) (1) (3), 0.032 (2) (1) (3)"]
["Opláštění","Barva","","","","","Bílá","Bílá","Bílá","Bílá","Bílá","","Bílá","Bílá","Bílá"]
["Rozměry","Jednotka","","Výška","mm","","215","289","215","298","215","","215","298","215"]
["","","","Šířka","mm","","780","780","780","900","900","","900","900","900"]
["","","","Hloubka","mm","","289","215","289","215","298","","298","215","298"]
["Hmotnost","Jednotka","","","kg","","8.00","8","8.00","11","11.0","","11.0","11","11.0"]
["Ventilátor","Průtok vzduchu","Chlazení","Vysoké","m³/min","","8.8","9.1","9.1","11.2","11.2","","11.2","11.9","11.9"]
["","","","Střední","m³/min","","6.7","7.0","7.0","","8.5","","9.1","","9.6"]
["","","","Nízký","m³/min","","4.7","5.0","5.0","5.8","5.8","","7.0","7.4","7.4"]
["","","","Tichý provoz","m³/min","","3.9","3.9","3.9","4.1","4.1","","4.1","4.5","4.5"]
["","","Vytápění","Vysoké","m³/min","","9.5","10.0","10.0","12.1","12.1","","12.4","13.3","13.3"]
["","","","Střední","m³/min","","7.8","8.0","8.0","","9.3","","10.0","","10.8"]
["","","","Nízký","m³/min","","6.0","6.0","6.0","6.5","6.5","","7.8","8.4","8.4"]
["","","","Tichý provoz","m³/min","","4.3","4.3","4.3","4.2","4.2","","5.2","5.5","5.5"]
["Hladina akustického výkonu","Chlazení","","","dBA","","58","58","58","59","59","","59","60","60"]
["","Vytápění","","","dBA","","58","58","58","59","59","","59","60","60"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","","40","41","41","45","45","","45","46","46"]
["","","","Střední","dBA","","32","33","33","","37","","39","","40"]
["","","","Nízký","dBA","","24","25","25","29","29","","33","34","34"]
["","","","Tichý provoz","dBA","","19","19","19","19","19","","21","23","23"]
["","Vytápění","","Vysoké","dBA","","40","41","41","45","45","","45","47","47"]
["","","","Střední","dBA","","34","34","34","","39","","39","","40"]
["","","","Nízký","dBA","","27","27","27","29","29","","33","34","34"]
["","","","Tichý provoz","dBA","","19","19","19","19","19","","22","24","24"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","","6.35","6.35","6.35","6.35","6.35","","6.35","6.35","6.35"]
["","Plyn","","Vnější průměr","mm","","9.50","9.5","9.50","9.5","9.50","","9.50","12.7","12.7"]
["","Odvod kondenzátu","","","","","18","18","18","18","18","","18","18","18"]
["Řídicí systémy","Infrared remote control","","","","","ARC466A6","","","","","","ARC466A9"]
["Standardní příslušenství","Installation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Wireless remote control","","","","","1","1","1","1","1","","1","1","1"]
["","AAA dry-cell batteries","","","","","2","","2","","2","","2","","2"]
["","Operation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2","","2","","2","","2"]
["","Indoor unit fixing screws","","","","","2","2","2","2","2","","2","2","2"]
["","Mounting plate","","","","","1","1","1","1","1","","1","1","1"]
["","Remote control holder","","","","","1","1","1","1","1","","1","1","1"]
["Napájení","Označení","","","","","V1","V1","V1","V1","V1","","V1","V1","V1"]
["","Fáze","","","","","1~","1~","1~","1~","1~","","1~","1~","1~"]
["","Frekvence","","","Hz","","50","50","50","50","50","","50","50","50"]
["","Napětí","","","V","","220-240","220-240","220-240","220-240","220-240","","220-240","220-240","220-240"]
["Ventilátor","Průtok vzduchu","Chlazení","Jm.","m³/min","","","9.1","","11.2","","","","11.9"]
["Hladina akustického tlaku","Chlazení","","Jm.","dBA","","","33","","37","","","","40"]
["Ventilátor","Průtok vzduchu","Vytápění","Jm.","m³/min","","","8.0","","9.3","","","","10.8"]
["Hladina akustického tlaku","Vytápění","","Jm.","dBA","","","34","","39","","","","40"]
["Řídicí systémy","Infračervené dálkové ovládání","","","","","","ARC466A6","ARC466A6","ARC466A6","ARC466A9","","","ARC466A6","ARC466A9"]
["Standardní příslušenství","Batteries","","","","","","2","","2","","","","2"]
["","Titanium apatite photocatalytic air purification filter","","","","","","2","","2","","","","2"]
["Poznámky","","","","","","","","","","","(4) - 240 V"]