{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":5,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-AW"]
[]
[]
[]
[]
["","","","","FTXTA30A2V1BW"]
["Hladina akustického tlaku","Vytápění","Vysoké","dBA","41"]
["","","Střední","dBA","31"]
["","","Tichý provoz","dBA","19"]
["","","Nízký","dBA","24"]
["","Chlazení","Střední","dBA","32"]
["","","Tichý provoz","dBA","20"]
["","","Nízký","dBA","25"]
["","","Vysoké","dBA","43"]
["Standardní příslušenství","Příručka pro instalaci","","","1"]
["","Manuální ovládání","","","1"]
["","Vzduchový filtr","","","2"]
["","Infračervené dálkové ovládání","","","1"]
["","Montážní deska dálkového ovládání","","","1"]
["","Sáček se šrouby","","","1"]
["","Krytka šroubu","","","2"]
["","Baterie AAA","","","2"]
["","Obecná bezpečnostní opatření","","","1"]
["Chladivo","Vliv na globální oteplování (GWP)","","","675.0"]
["Řídicí systémy","Wired remote control","","","BRC073A4"]
["","Infrared remote control","","","ARC466A59"]
["Piping connections","Kapalina","Vnější průměr","mm","6.35"]
["","Plyn","Vnější průměr","mm","9.50"]
["","Vypouštění","","","18"]
["Příkon","Chlazení","Jm.","kW","0.023"]
["","Vytápění","Jm.","kW","0.022"]
["Hladina akustického výkonu","Chlazení","","dBA","60"]
["","Vytápění","","dBA","60"]
["Rozměry","Jednotka","Šířka","mm","798"]
["","","Hloubka","mm","189"]
["","","Výška","mm","295"]
["Opláštění","Colour","","","Bílý"]
["Hmotnost","Jednotka","","kg","11.5"]
["Power supply","Phase","","","1~"]
["","Frekvence","","Hz","50"]
["","Označení","","","V1"]
["","Napětí","","V","220-240"]