{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":6,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-CB"]
[]
[]
[]
[]
["","","","","","FTXTA30C2V1BB"]
["Vstup napájení","Chlazení","","Jm.","kW","0.023"]
["","Vytápění","","Jm.","kW","0.022"]
["Opláštění","Barva","","","","Černá"]
["Rozměry","Jednotka","","Výška","mm","295"]
["","","","Šířka","mm","798"]
["","","","Hloubka","mm","189"]
["Hmotnost","Jednotka","","","kg","12"]
["Ventilátor","Průtok vzduchu","Chlazení","Vysoké","m³/min","13.1"]
["","","","Střední","m³/min","9"]
["","","","Nízký","m³/min","6"]
["","","","Tichý provoz","m³/min","4.9"]
["","","Vytápění","Vysoké","m³/min","12.3"]
["","","","Střední","m³/min","8.2"]
["","","","Nízký","m³/min","5.8"]
["","","","Tichý provoz","m³/min","5"]
["Hladina akustického výkonu","Chlazení","","","dBA","60"]
["","Vytápění","","","dBA","60"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","43"]
["","","","Střední","dBA","32"]
["","","","Nízký","dBA","25"]
["","","","Tichý provoz","dBA","20"]
["","Vytápění","","Vysoké","dBA","41"]
["","","","Střední","dBA","31"]
["","","","Nízký","dBA","24"]
["","","","Tichý provoz","dBA","19"]
["Chladivo","Vliv na globální oteplování (GWP)","","","","675"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","6.35"]
["","Plyn","","Vnější průměr","mm","9.5"]
["","Odvod kondenzátu","","","","18"]
["Řídicí systémy","Infrared remote control","","","","ARC466A84"]
["Řídicí systémy","Kabelové dálkové ovládání","","","","BRC073A4"]
["Standardní příslušenství","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","Screw cover","","","","2"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","1"]
["","Silver particle filter","","","","1"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Napájení","Fáze","","","","1~"]
["","Frekvence","","","Hz","50"]
["","Napětí","","","V","220-240"]