{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-A / RXTM-A"]
[]
[]
[]
[]
["","","","","FTXTM30A2V1B / RXTM30A2V1B","FTXTM40A2V1B / RXTM40A2V1B"]
["Chladicí výkon","Min.","","kW","1.2","1.2"]
["","Jm.","","kW","3","4"]
["","Max.","","kW","4.6","5.2"]
["Topný výkon","Min.","","kW","0.8","0.9"]
["","Jm.","","kW","3.2","4"]
["","Max.","","kW","7.4","8.8"]
["Jmenovitá účinnost","EER","","","5.13","4.71"]
["","COP","","","5.3","5.51"]
["","Roční spotřeba energie","","kWh","292","425"]
["","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích-=-Chlazení","","A","A"]
["","","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích-=-Vytápění","","A","A"]
["Prostorové chlazení","Třída energetické úspornosti","","","A+++","A+++"]
["","Kapacita","Pnávrh","kW","3","4"]
["","SEER","","","8.65","8.95"]
["","Roční spotřeba energie","","kWh/a","121","156"]
["Prostorové vytápění (průměrné klima)","Třída energetické účinnosti","","","A+++","A+++"]
["","Výkon","Pnávrh","kW","3","3.8"]
["","SCOP/A","","","5.35","5.5"]
["","Topný výkon Pdh při -10°","","kW","3","3.8"]
["","Roční spotřeba energie","","kWh/a","785","967"]
["Energetickou účinná řada","","","","A+++ ~ D","A+++ ~ D"]
["Poznámky","","","","(1) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m.","(1) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]
["","","","","(2) - Jmenovité chladicí výkony vycházejí ztěchto podmínek: vnitřní tep.: 27°CDB, 19°CWB, venkovní teplota: 35°CDB, ekvivalentní délka potrubí schladivem: 5m, rozdíl úrovní: 0m.","(2) - Jmenovité chladicí výkony vycházejí ztěchto podmínek: vnitřní tep.: 27°CDB, 19°CWB, venkovní teplota: 35°CDB, ekvivalentní délka potrubí schladivem: 5m, rozdíl úrovní: 0m."]
["","","","","(3) - Viz samostatný výkres s provozním rozsahem","(3) - Viz samostatný výkres s provozním rozsahem"]
["","","","","(4) - Údaje o elektrickém systému najdete v samostatném výkresu","(4) - Údaje o elektrickém systému najdete v samostatném výkresu"]