{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-A"]
[]
[]
[]
[]
["","","","","","FTXTM30A2V1B","FTXTM40A2V1B"]
["Vstup napájení","Chlazení","","Jm.","kW","0.029","0.053"]
["","Vytápění","","Jm.","kW","0.024","0.06"]
["Opláštění","Barva","","","","Bílá","Bílá"]
["Rozměry","Jednotka","","Výška","mm","298","298"]
["","","","Šířka","mm","804","997"]
["","","","Hloubka","mm","252","292"]
["Hmotnost","Jednotka","","","kg","12","15"]
["Ventilátor","Průtok vzduchu","Chlazení","Vysoké","m³/min","13.2","15.1"]
["","","","Střední","m³/min","8.1","9.2"]
["","","","Nízký","m³/min","5.6","5.6"]
["","","","Tichý provoz","m³/min","4.8","4.8"]
["","","Vytápění","Vysoké","m³/min","11.7","17"]
["","","","Střední","m³/min","7.7","10"]
["","","","Nízký","m³/min","5.6","6"]
["","","","Tichý provoz","m³/min","4.7","5.1"]
["Hladina akustického výkonu","Chlazení","","","dBA","60","60"]
["","Vytápění","","","dBA","59","60"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","45","46"]
["","","","Střední","dBA","33","32"]
["","","","Nízký","dBA","25","24"]
["","","","Tichý provoz","dBA","21","20"]
["","Vytápění","","Vysoké","dBA","43","46"]
["","","","Střední","dBA","31","31"]
["","","","Nízký","dBA","22","22"]
["","","","Tichý provoz","dBA","19","19"]
["Chladivo","Vliv na globální oteplování (GWP)","","","","675","675"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","6.35","6.35"]
["","Plyn","","Vnější průměr","mm","9.5","9.5"]
["","Odvod kondenzátu","","","","18","18"]
["Řídicí systémy","Infračervené dálkové ovládání","","","","ARC466A83","ARC466A83"]
["Standardní příslušenství","FTXTM30A2V1B","","","","1"]
["","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","Screw cover","","","","2","2"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Napájení","Označení","","","","V1","V1"]
["","Fáze","","","","1~","1~"]
["","Frekvence","","","Hz","50","50"]
["","Napětí","","","V","220-240","220-240"]
["Poznámky","","","","","(1) - Køling: indendørs temp: 27 °CDB, 19 °CWB, udendørs temp. 35°CDB, 24°CWB; tilsvarende rørlængde: 5 m","(1) - Køling: indendørs temp: 27 °CDB, 19 °CWB, udendørs temp. 35°CDB, 24°CWB; tilsvarende rørlængde: 5 m"]
["","","","","","(2) - Vytápění: vnitřní teplota 20° CDB; vnější teplota 7° CDB, 6° CWB ekvivalentní délka potrubí chladiva: 5m","(2) - Vytápění: vnitřní teplota 20° CDB; vnější teplota 7° CDB, 6° CWB ekvivalentní délka potrubí chladiva: 5m"]
["","","","","","(3) - Údaje o elektrickém systému najdete v samostatném výkresu","(3) - Údaje o elektrickém systému najdete v samostatném výkresu"]
["Standardní příslušenství","FTXTM40A2V1B","","","","","1"]