{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":94,"n_cols":7,"rows_kept":94,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-R"]
[]
[]
[]
[]
["","","","","","FTXTM30R2V1B","FTXTM40R2V1B"]
["Hladina akustického tlaku","Vytápění","","Vysoké","dBA","45.0"]
["","","","Střední","dBA","31.0"]
["","","","Tichý provoz","dBA","19.0"]
["","","","Nízký","dBA","22.0"]
["","Chlazení","","Střední","dBA","33.0"]
["","","","Tichý provoz","dBA","21.0"]
["","","","Nízký","dBA","25.0"]
["","","","Vysoké","dBA","45.0"]
["Standardní příslušenství","Příručka pro instalaci","","","","1"]
["","Manuální ovládání","","","","1"]
["","Bezdrátové dálkové ovládání","","","","1"]
["","Baterie AAA","","","","2"]
["","Držák dálkového ovládání","","","","1"]
["","Montážní deska","","","","1"]
["","Upevňovací šrouby vnitřní jednotky","","","","2"]
["","Stříbrný filtr částic","","","","1"]
["Řídicí systémy","Kabelové dálkové ovládání","","","","BRC073A1"]
["","Infrared remote control","","","","ARC466A75"]
["Spoje potrubí","Kapalina","","Vnější průměr","mm","6.35"]
["","Plyn","","Vnější průměr","mm","9.50"]
["","Vypouštění","","","","18"]
["Příkon","Chlazení","","Jm.","kW","0.035"]
["","Vytápění","","Jm.","kW","0.039"]
["Sound power level","Chlazení","","","dBA","60.0"]
["","Vytápění","","","dBA","61.0"]
["Rozměry","Jednotka","","Šířka","mm","778"]
["","","","Hloubka","mm","272"]
["","","","Výška","mm","295"]
["Opláštění","Barva","","","","Bílý"]
["Hmotnost","Jednotka","","","kg","10.0"]
["Ventilátor","Průtok vzduchu","Vytápění","Vysoké","m³/min","12.5"]
["","","","Nízký","m³/min","4.9"]
["","","","Střední","m³/min","7.5"]
["","","","Tichý provoz","m³/min","4.0"]
["","","Chlazení","Nízký","m³/min","5.3"]
["","","","Střední","m³/min","7.8"]
["","","","Vysoké","m³/min","12.2"]
["","","","Tichý provoz","m³/min","4.1"]
["Power supply","Fáze","","","","1~"]
["","Frekvence","","","Hz","50"]
["","Označení","","","","V1"]
["","Napětí","","","V","220-240"]
["Poznámky","","","","","(1) - Køling: indendørs temp: 27 °CDB, 19,0 °CWB; udendørs temp. 35°CDB, 24°CWB; tilsvarende rørlængde: 5m"]
["","","","","","(2) - Vytápění: vnitřní teplota 20° CDB; vnější teplota 7° CDB, 6° CWB ekvivalentní délka potrubí chladiva: 5m"]
["","","","","","(3) - Údaje o elektrickém systému najdete na zvláštním schématu"]
["Vstup napájení","Chlazení","","Jm.","kW","","0.053"]
["","Vytápění","","Jm.","kW","","0.06"]
["Opláštění","Barva","","","","","Bílá"]
["Rozměry","Jednotka","","Výška","mm","","299"]
["","","","Šířka","mm","","998"]
["","","","Hloubka","mm","","292"]
["Hmotnost","Jednotka","","","kg","","14.5"]
["Ventilátor","Průtok vzduchu","Chlazení","Vysoké","m³/min","","15.4"]
["","","","Střední","m³/min","","9.5"]
["","","","Nízký","m³/min","","5.8"]
["","","","Tichý provoz","m³/min","","4.6"]
["","","Vytápění","Vysoké","m³/min","","17.5"]
["","","","Střední","m³/min","","10.5"]
["","","","Nízký","m³/min","","7.1"]
["","","","Tichý provoz","m³/min","","5.9"]
["Hladina akustického výkonu","Chlazení","","","dBA","","60"]
["","Vytápění","","","dBA","","61"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","","46"]
["","","","Střední","dBA","","32"]
["","","","Nízký","dBA","","24"]
["","","","Tichý provoz","dBA","","20"]
["","Vytápění","","Vysoké","dBA","","46"]
["","","","Střední","dBA","","31"]
["","","","Nízký","dBA","","22"]
["","","","Tichý provoz","dBA","","19"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","","6.35"]
["","Plyn","","Vnější průměr","mm","","9.5"]
["","Odvod kondenzátu","","","","","18"]
["Řídicí systémy","Infrared remote control","","","","","ARC466A75"]
["Řídicí systémy","Kabelové dálkové ovládání","","","","","BRC073A1"]
["Standardní příslušenství","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","1"]
["","Silver particle filter","","","","","1"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Napájení","Označení","","","","","V1"]
["","Fáze","","","","","1~"]
["","Frekvence","","","Hz","","50"]
["","Napětí","","","V","","220-240"]