{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":83,"n_cols":7,"rows_kept":83,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-K"]
[]
[]
[]
[]
["","","","","","FTXTP25K3V1B","FTXTP35K3V1B"]
["Hladina akustického tlaku","Vytápění","","Vysoké","dBA","43"]
["","","","Střední","dBA","35"]
["","","","Tichý provoz","dBA","21"]
["","","","Nízký","dBA","26"]
["","Chlazení","","Medium","dBA","35"]
["","","","Tichý provoz","dBA","21"]
["","","","Nízký","dBA","26"]
["","","","Vysoké","dBA","43"]
["Standardní příslušenství","Příručka pro instalaci","","","","1"]
["","Manuální ovládání","","","","1"]
["","Bezdrátové dálkové ovládání","","","","1"]
["","Baterie AAA","","","","2"]
["","Držák dálkového ovládání","","","","1"]
["","Montážní deska","","","","1"]
["","Deodorizační filtr s apatitem titanu","","","","2"]
["","Upevňovací šrouby vnitřní jednotky","","","","2"]
["Control systems","Wired remote control","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","ARC480A11"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","6.35"]
["","Plyn","","Vnější průměr","mm","9.50"]
["","Vypouštění","","","","16 (vnitřní průměr připojované hadice)"]
["Vstup napájení","Chlazení","","Jm.","kW","0.030"]
["","Vytápění","","Jm.","kW","0.035"]
["Hladina akustického výkonu","Chlazení","","","dBA","58"]
["","Vytápění","","","dBA","58"]
["Rozměry","Jednotka","","Šířka","mm","770"]
["","","","Hloubka","mm","225"]
["","","","Výška","mm","285"]
["Casing","Colour","","","","Bílý"]
["Hmotnost","Jednotka","","","kg","9.0"]
["Power supply","Phase","","","","1~"]
["","Frekvence","","","Hz","50"]
["","Name","","","","V1"]
["","Napětí","","","V","220-240"]
["Poznámky","","","","","(1) - Údaje o elektrickém systému najdete v samostatném výkresu"]
["Vstup napájení","Chlazení","","Jm.","kW","","0.03"]
["","Vytápění","","Jm.","kW","","0.035"]
["Opláštění","Barva","","","","","Bílá"]
["Rozměry","Jednotka","","Výška","mm","","285"]
["","","","Šířka","mm","","770"]
["","","","Hloubka","mm","","225"]
["Hmotnost","Jednotka","","","kg","","9"]
["Ventilátor","Průtok vzduchu","Chlazení","Vysoké","m³/min","","11.4"]
["","","","Střední","m³/min","","8.2"]
["","","","Nízký","m³/min","","5.4"]
["","","","Tichý provoz","m³/min","","4.3"]
["","","Vytápění","Vysoké","m³/min","","10.8"]
["","","","Střední","m³/min","","7.8"]
["","","","Nízký","m³/min","","5.8"]
["","","","Tichý provoz","m³/min","","4.9"]
["Hladina akustického výkonu","Chlazení","","","dBA","","58"]
["","Vytápění","","","dBA","","58"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","","43"]
["","","","Střední","dBA","","35"]
["","","","Nízký","dBA","","26"]
["","","","Tichý provoz","dBA","","21"]
["","Vytápění","","Vysoké","dBA","","43"]
["","","","Střední","dBA","","35"]
["","","","Nízký","dBA","","26"]
["","","","Tichý provoz","dBA","","21"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","","6.35"]
["","Plyn","","Vnější průměr","mm","","9.5"]
["","Odvod kondenzátu","","","","","16 (vnitřní průměr připojované hadice)"]
["Control systems","Infrared remote control","","","","","ARC480A11"]
["Řídicí systémy","Kabelové dálkové ovládání","","","","","BRC944B2, BRC073A1"]
["Standardní příslušenství","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","2"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Napájení","Označení","","","","","V1"]
["","Fáze","","","","","1~"]
["","Frekvence","","","Hz","","50"]
["","Napětí","","","V","","220-240"]