{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":82,"n_cols":11,"rows_kept":82,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A"]
[]
[]
[]
[]
["","","","","","FUA71AVEB9","FUA100AVEB9","FUA125AVEB9","FUA71AVEB (Archived)","FUA100AVEB (Archived)","FUA125AVEB (Archived)"]
["Hladina akustického tlaku","Vytápění","","Vysoké","dBA","","","","41","46","47"]
["","","","Střední","dBA","","","","38","42","43"]
["","","","Nízký","dBA","","","","35","39","40"]
["","Chlazení","","Střední","dBA","","","","38","42","43"]
["","","","Nízký","dBA","","","","35","39","40"]
["","","","Vysoké","dBA","","","","41","46","47"]
["Standardní příslušenství","Manuální ovládání","","","","","","","1","1","1"]
["","Příručka pro instalaci","","","","","","","1","1","1"]
["","Drenážní hadice","","","","","","","1","1","1"]
["","Tepelná izolační trubka","","","","","","","3","3","3"]
["","Spojky pláště","","","","","","","10","10","10"]
["","Hadicová páska","","","","","","","1","1","1"]
["","Těsnící materiál","","","","","","","4","4","4"]
["","Upínací deska podložky","","","","","","","1","1","1"]
["","Spoj vypouštění","","","","","","","1","1","1"]
["","Netkaná textilie","","","","","","","1","1","1"]
["","Podložka","","","","","","","8","8","8"]
["","Upínací šroub pro vypouštěcí hadici","","","","","","","5","5","5"]
["Řídicí systémy","Wired remote control","","","","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Chladicí výkon","Total capacity","","Jm.","kW","","","","","","12.1"]
["Spoje potrubí","Liquid","","OD","mm","","","","9.52","9.52","9.52"]
["","Plyn","","OD","mm","","","","15.9","15.9","15.9"]
["","Vypouštění","","","","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Hladina akustického výkonu","Chlazení","","","dBA","","","","59","64","65"]
["","Vytápění","","","dBA","","","","59","64"]
["Rozměry","Jednotka","","Šířka","mm","","","","950","950","950"]
["","","","Hloubka","mm","","","","950","950","950"]
["","","","Výška","mm","","","","198","198","198"]
["Casing","Material","","","","","","","Pryskyřice","Pryskyřice","Pryskyřice"]
["","Barva","","","","","","","Čerstvý bílý","Čerstvý bílý","Čerstvý bílý"]
["Hmotnost","Jednotka","","","kg","","","","25.0","26.0","26"]
["Ventilátor","Průtok vzduchu","Vytápění","Vysoké","m³/min","","","","23.0","31.0","32.5"]
["","","","Medium","m³/min","","","","19.5","25.5","26.5"]
["","","","Nízký","m³/min","","","","16.0","20.0","20.5"]
["","","Chlazení","Nízký","m³/min","","","","16.0","20.0","20.5"]
["","","","Medium","m³/min","","","","19.5","25.5","26.5"]
["","","","Vysoké","m³/min","","","","23.0","31.0","32.5"]
["Hladina vypouštění","mm","","","","","","","600","600","600"]
["Topný výkon","Total capacity","","Jmen.","kW","","","","","","13.5"]
["Opláštění","Barva","","","","Čerstvý bílý","Čerstvý bílý","Čerstvý bílý"]
["","Materiál","","","","Pryskyřice","Pryskyřice","Pryskyřice"]
["Rozměry","Jednotka","","Výška","mm","198","198","198"]
["","","","Šířka","mm","950","950","950"]
["","","","Hloubka","mm","950","950","950"]
["Hmotnost","Jednotka","","","kg","25.0","26.0","26.0"]
["Ventilátor","Průtok vzduchu","Chlazení","Vysoké","m³/min","23.0","31.0","32.5"]
["","","","Střední","m³/min","19.5","25.5","26.5"]
["","","","Nízký","m³/min","16.0","20.0","20.5"]
["","","Vytápění","Vysoké","m³/min","23.0","31.0","32.5"]
["","","","Střední","m³/min","19.5","25.5","26.5"]
["","","","Nízký","m³/min","16.0","20.0","20.5"]
["Hladina akustického výkonu","Chlazení","","","dBA","59","64","65"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","41","46","47"]
["","","","Střední","dBA","38","42","43"]
["","","","Nízký","dBA","35","39","40"]
["","Vytápění","","Vysoké","dBA","41","46","47"]
["","","","Střední","dBA","38","42","43"]
["","","","Nízký","dBA","35","39","40"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","9.52","9.52","9.52"]
["","Plyn","","Vnější průměr","mm","15.9","15.9","15.9"]
["","Odvod kondenzátu","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Hladina vypouštění","mm","","","","600","600","600"]
["Standardní příslušenství","Installation manual","","","","1","1","1"]
["","Thermal insulation tube","","","","3","3","3"]
["","Non woven fabric","","","","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Hose band","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Drain hose","","","","1","1","1"]
["","Fixing screw for drain hose","","","","5","5","5"]
["","Sealing material","","","","4","4","4"]
["","Tie-wraps","","","","10","10","10"]
["","Washer","","","","8","8","8"]
["","Washer fixing plate","","","","1","1","1"]
["Chladicí výkon","Celkový výkon","","Jm.","kW","","","12.10"]
["Topný výkon","Celkový výkon","","Jmen.","kW","","","13.5"]