{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":7,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUQ-C"]
[]
[]
[]
[]
["","","","","FUQ71CVEB","FUQ100CVEB","FUQ125CVEB"]
["Hladina akustického tlaku","Vytápění","Vysoké","dBA","41","46","47"]
["","","Jm.","dBA","38","42","43"]
["","","Nízký","dBA","35","39","40"]
["","Chlazení","Nízký","dBA","35","39","40"]
["","","Vysoké","dBA","41","46","47"]
["","","Jm.","dBA","38","42","43"]
["Standardní příslušenství","Příručka pro instalaci","","","Příručka pro instalaci","Příručka pro instalaci","Příručka pro instalaci"]
["","Manuální ovládání","","","Manuální ovládání","Manuální ovládání","Manuální ovládání"]
["","Prohlášení o shodě","","","Prohlášení o shodě","Prohlášení o shodě","Prohlášení o shodě"]
["","Drenážní hadice","","","Drenážní hadice","Drenážní hadice","Drenážní hadice"]
["","Kovová svorka","","","Kovová svorka","Kovová svorka","Kovová svorka"]
["","Podložka pro konzoli závěsu","","","Podložka pro konzoli závěsu","Podložka pro konzoli závěsu","Podložka pro konzoli závěsu"]
["","Svorky","","","Svorky","Svorky","Svorky"]
["","Podložka","","","Podložka","Podložka","Podložka"]
["","Materiál pro izolaci a těsnění spojů","","","Materiál pro izolaci a těsnění spojů","Materiál pro izolaci a těsnění spojů","Materiál pro izolaci a těsnění spojů"]
["","Koleno","","","Koleno","Koleno","Koleno"]
["","Instalační šablona","","","Instalační šablona","Instalační šablona","Instalační šablona"]
["","Blokovací materiál","","","Blokovací materiál","Blokovací materiál","Blokovací materiál"]
["","Potrubí ve tvaru L","","","Potrubí ve tvaru L","Potrubí ve tvaru L","Potrubí ve tvaru L"]
["","Šrouby","","","Šrouby","Šrouby","Šrouby"]
["","Netkaná textilie","","","Netkaná textilie","Netkaná textilie","Netkaná textilie"]
["Řídicí systémy","Wired remote control","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","BRC7C58","BRC7C58","BRC7C58"]
["Připojovací rozměry","Kapalina","Vnější průměr","mm","9.52","9.52","9.52"]
["","Plyn","Vnější průměr","mm","15.9","15.9","15.9"]
["","Vypouštění","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Sound power level","Chlazení","","dBA","59","64","65"]
["","Vytápění","","dBA","59","64","65"]
["Rozměry","Jednotka","Šířka","mm","950","950","950"]
["","","Hloubka","mm","950","950","950"]
["","","Výška","mm","198","198","198"]
["Opláštění","Materiál","","","Pryskyřice","Pryskyřice","Pryskyřice"]
["","Barva","","","Čerstvý bílý","Čerstvý bílý","Čerstvý bílý"]
["Hmotnost","Jednotka","","kg","25","26","26"]
["Hladina vypouštění","mm","","","600","600","600"]
["Power supply","Fáze","","","1~","1~","1~"]
["","Frekvence","","Hz","50/60","50/60","50/60"]
["","Označení","","","VE","VE","VE"]
["","Napětí","","V","220-240/220","220-240/220","220-240/220"]