{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":7,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVQ-C / RZQG-L8/7V1"]
[]
[]
[]
[]
["","","","","FVQ71CVEB / RZQG71L8V1B","FVQ100CVEB / RZQG100L8V1B","FVQ125CVEB / RZQG125L8V1B"]
["Chladicí výkon","Jm.","","kW","6.8","","12.0"]
["Prostorové chlazení","SEER","","","6.31","","5.61"]
["","Roční spotřeba energie","","kWh/a","377.179","","748.663"]
["","Kapacita","Pnávrh","kW","6.80","","12.00"]
["","Třída energetické úspornosti","","","A++","","A+"]
["Prostorové vytápění (průměrné klima)","Výkon","Pnávrh","kW","6.33","","11.30"]
["","SCOP/A","","","4.05","","3.87"]
["","Třída energetické účinnosti","","","A+","","A"]
["","Roční spotřeba energie","","kWh/a","2,188.148","","4,087.855"]
["Jmenovitá účinnost","Annual energy consumption","","kWh","1,010","","1,870"]
["","EER","","","3.37","","3.21"]
["","COP","","","3.64","","3.70"]
["","Směrnice o energetických štítcích","Chlazení","","A","","A"]
["","","Vytápění","","A","","A"]
["Topný výkon","Jm.","","kW","7.5","","13.5"]
["Poznámky","","","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU"]
["","","","","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení"]