{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":7,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXG-K / RXG-L"]
[]
[]
[]
[]
["","","","","FVXG25K2V1B / RXG25L2V1B","FVXG35K2V1B / RXG35L2V1B","FVXG50K2V1B / RXG50L2V1B"]
["Chladicí výkon","Min.","","kW","1.3","1.4","1.7"]
["","Jm.","","kW","2.5","3.5","5.0"]
["","Max.","","kW","3.0","3.8","5.6"]
["Topný výkon","Min.","","kW","1.3","1.4","1.7"]
["","Jm.","","kW","3.4","4.5","5.8"]
["","Max.","","kW","4.5","5.0","8.1"]
["Jmenovitá účinnost","EER","","","4.63","3.72","3.31"]
["","COP","","","4.42","3.75","3.69"]
["","Roční spotřeba energie","","kWh","270","470","755"]
["","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích-=-Chlazení","","A","A","A"]
["","","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích-=-Vytápění","","A","A","A"]
["Připojovací rozměry","Plyn","Vnější průměr","mm","9.5","9.5","12.7"]
["","Kapalina","Vnější průměr","mm","6.35","6.35","6.35"]
["Prostorové chlazení","Třída energetické úspornosti","","","A++","A++","A"]
["","Kapacita","Pnávrh","kW","2.50","3.50","5.00"]
["","SEER","","","6.53","6.48","5.41"]
["","Roční spotřeba energie","","kWh/r","134","189","324"]
["Prostorové vytápění (průměrné klima)","Třída energetické účinnosti","","","A++","A+","A+"]
["","Výkon","Pnávrh","kW","2.80","3.10","4.60"]
["","SCOP/A","","","4.65","4.00","4.18"]
["","Roční spotřeba energie","","kWh/r","842","1087","1543"]
["Poznámky","","","","(1) - Chlazení pokojová teplota 27°CST, 19°CMT; venkovní teplota 35°CST, 24°CMT","(1) - Chlazení pokojová teplota 27°CST, 19°CMT; venkovní teplota 35°CST, 24°CMT","(1) - Chlazení pokojová teplota 27°CST, 19°CMT; venkovní teplota 35°CST, 24°CMT"]
["","","","","(2) - Vytápění: vnitřní teplota 20° CDB; vnější teplota 7°CDB, 6°CWB","(2) - Vytápění: vnitřní teplota 20° CDB; vnější teplota 7°CDB, 6°CWB","(2) - Vytápění: vnitřní teplota 20° CDB; vnější teplota 7°CDB, 6°CWB"]