{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":8,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-A9"]
[]
[]
[]
[]
["","","","","","FVXM25A3V1B9","FVXM35A3V1B9","FVXM50A3V1B9"]
["Vstup napájení","Chlazení","","Jm.","kW","0.02","0.02","0.03"]
["","Vytápění","","Jm.","kW","0.02","0.03","0.03"]
["Opláštění","Barva","","","","Bílá","Bílá","Bílá"]
["Rozměry","Jednotka","","Výška","mm","600","600","600"]
["","","","Šířka","mm","750","750","750"]
["","","","Hloubka","mm","238","238","238"]
["Hmotnost","Jednotka","","","kg","17","17","17"]
["Ventilátor","Průtok vzduchu","Chlazení","Vysoké","m³/min","8.7","9.2","11.6"]
["","","","Střední","m³/min","7","7","9"]
["","","","Nízký","m³/min","4.9","4.9","6.6"]
["","","","Tichý provoz","m³/min","4.1","4.1","5.4"]
["","","Vytápění","Vysoké","m³/min","9.2","9.8","12.8"]
["","","","Střední","m³/min","7.2","7.2","10"]
["","","","Nízký","m³/min","5.6","5.6","8.4"]
["","","","Tichý provoz","m³/min","4.1","4.1","5.9"]
["Hladina akustického výkonu","Chlazení","","","dBA","52","53","61"]
["","Vytápění","","","dBA","52","53","62"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","38","39","44"]
["","","","Střední","dBA","32","32","38"]
["","","","Nízký","dBA","25","25","31"]
["","","","Tichý provoz","dBA","20","20","27"]
["","Vytápění","","Vysoké","dBA","38","39","46"]
["","","","Střední","dBA","32","32","40"]
["","","","Nízký","dBA","25","25","35"]
["","","","Tichý provoz","dBA","19","19","29"]
["Chladivo","Vliv na globální oteplování (GWP)","","","","675","675","675"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","6.4","6.4","6.4"]
["","Plyn","","Vnější průměr","mm","9.5","9.5","12.7"]
["","Odvod kondenzátu","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Řídicí systémy","Infračervené dálkové ovládání","","","","ARC466A66","ARC466A66","ARC466A66"]
["","Kabelové dálkové ovládání","","","","BRC073A1","BRC073A1","BRC073A1"]
["Napájení","Fáze","","","","1~","1~","1~"]
["","Frekvence","","","Hz","50","50","50"]
["","Napětí","","","V","220-240","220-240","220-240"]
["Standardní příslušenství","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","General safety precautions","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Remote control holder","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Energetickou účinná řada","","","","","A+++ ~ D"]
["Poznámky","","","","","(1) - Køling: indendørs temp: 27 °CDB, 19 °CWB, udendørs temp. 35°CDB, 24°CWB; tilsvarende rørlængde: 5 m"]
["","","","","","(2) - Vytápění: vnitřní teplota 20° CDB; vnější teplota 7° CDB, 6° CWB ekvivalentní délka potrubí chladiva: 5m"]