{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXTM-B / RXTM-A"]
[]
[]
[]
[]
["","","","","FVXTM30B2V1B / RXTM30A2V1B"]
["Chladicí výkon","Min.","","kW","1.2"]
["","Jm.","","kW","3"]
["","Max.","","kW","4.4"]
["Topný výkon","Min.","","kW","1.2"]
["","Jm.","","kW","3.2"]
["","Max.","","kW","6.2"]
["Jmenovitá účinnost","EER","","","4.35"]
["","COP","","","4.45"]
["","Roční spotřeba energie","","kWh","345"]
["","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích-=-Chlazení","","A"]
["","","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích-=-Vytápění","","A"]
["Prostorové chlazení","Třída energetické úspornosti","","","A++"]
["","Kapacita","Pnávrh","kW","3"]
["","SEER","","","7.5"]
["","Roční spotřeba energie","","kWh/a","140"]
["Prostorové vytápění (průměrné klima)","Třída energetické účinnosti","","","A++"]
["","Výkon","Pnávrh","kW","3"]
["","SCOP/A","","","4.75"]
["","Topný výkon Pdh při -10°","","kW","3"]
["","Roční spotřeba energie","","kWh/a","884"]
["Poznámky","","","","(1) - Údaje o elektrickém systému najdete v samostatném výkresu"]
["","","","","(2) - Viz samostatný výkres s provozním rozsahem"]
["","","","","(3) - Jmenovité chladicí výkony vycházejí z těchto podmínek: vnitřní tep.: 27°CDB, 19°CWB, venkovní teplota: 35 °CDB, ekvivalentní délka potrubí s chladivem: 5 m, rozdíl úrovní: 0 m."]
["","","","","(4) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]