{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":77,"n_cols":11,"rows_kept":77,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FWXT-ATV3"]
[]
[]
[]
[]
["","","","","","FWXT10ABTV3","FWXT15ABTV3","FWXT20ABTV3","FWXT10AATV3 (Archived)","FWXT15AATV3 (Archived)","FWXT20AATV3 (Archived)"]
["Rozměry","Jednotka","","Šířka","mm","","","","902","1,100","1,300"]
["","","","Hloubka","mm","","","","128","128","128"]
["","","","Výška","mm","","","","335","335","335"]
["Opláštění","Barva","","","","","","","RAL 9003","RAL 9003","RAL 9003"]
["Hmotnost","Jednotka","","","kg","","","","14.0","16.0","19.0"]
["Power supply","Fáze","","","","","","","1~","1~","1~"]
["","Frekvence","","","Hz","","","","50","50","50"]
["","Napětí","","","V","","","","230","230","230"]
["Chladicí výkon","Chladicí výkon-=-7/12&nbsp;°C","","Chladicí výkon-=-7/12&nbsp;°C-=-Min.-=-kW","kW","0.49","0.62","0.70"]
["","","","Chladicí výkon-=-7/12&nbsp;°C-=-Stř.-=-kW","kW","0.88","1.08","1.21"]
["","","","Chladicí výkon-=-7/12&nbsp;°C-=-Max.-=-kW","kW","1.24","1.61","1.94"]
["Pocitový chladicí výkon","Pocitový chladicí výkon-=-7/12&nbsp;°C","","Pocitový chladicí výkon-=-7/12&nbsp;°C-=-Min.-=-kW","kW","0.37","0.52","0.57"]
["","","","Pocitový chladicí výkon-=-7/12&nbsp;°C-=-Stř.-=-kW","kW","0.70","0.86","1.02"]
["","","","Pocitový chladicí výkon-=-7/12&nbsp;°C-=-Max.-=-kW","kW","0.98","1.27","1.52"]
["Topný výkon","Topný výkon-=-45/40&nbsp;°C","","Topný výkon-=-45/40&nbsp;°C-=-Min.-=-kW","kW","0.55","0.79","0.74"]
["","","","Topný výkon-=-45/40&nbsp;°C-=-Stř.-=-kW","kW","1.00","1.36","1.55"]
["","","","Topný výkon-=-45/40&nbsp;°C-=-Max.-=-kW","kW","1.50","2.01","2.13"]
["Příkon","Min.","","","kW","0.01","0.01","0.01"]
["","Stř.","","","kW","0.01","0.01","0.01"]
["","Max.","","","kW","0.02","0.02","0.03"]
["Otáčky ventilátoru","Min.","","","ot./min","680.00","680.00","680.00"]
["","Stř.","","","ot./min","1100.00","1100.00","1100.00"]
["","Max.","","","ot./min","1500.00","1500.00","1500.00"]
["Opláštění","Barva","","","","RAL 9003","RAL 9003","RAL 9003"]
["","Materiál","","","","Plech","Plech","Plech"]
["Rozměry","Jednotka","","Výška","mm","335","335","335"]
["","","","Šířka","mm","902","1102","1302"]
["","","","Hloubka","mm","128","128","128"]
["","Jednotka v obalu","","Výška","mm","490","490","490"]
["","","","Šířka","mm","1030","1230","1430"]
["","","","Hloubka","mm","210","210","210"]
["Hmotnost","Jednotka","","","kg","14","16","19"]
["","Jednotka v obalu","","","kg","15","17","20"]
["Balení","Materiál","","","","Kartón","Kartón","Kartón"]
["","Hmotnost","","","kg","1","1","1"]
["Tepelný výměník","Množství","","","","1","1","1"]
["","Vnitřní objem výparníku","","","l","0.5","0.61","0.77"]
["","Plnění","","Provozní tlak","bar","10","10","10"]
["Vodní okruh","Průměr trubkového připojení","","","in","3/4","3/4","3/4"]
["","Potrubní materiál","","","","MĚĎ","MĚĎ","MĚĎ"]
["","Tlak","Vytápění","Max.","bar","10","10","10"]
["Vodní okruh – pokles tlaku vody","Vytápění","Vodní okruh – pokles tlaku vody-=-Vytápění-=-45/40&nbsp;°C","Vodní okruh – pokles tlaku vody-=-Vytápění-=-45/40&nbsp;°C-=-Min.-=-kPa","kPa","5.10","4.81","6.00"]
["","","","Vodní okruh – pokles tlaku vody-=-Vytápění-=-45/40&nbsp;°C-=-Stř.-=-kPa","kPa","12.00","6.30","6.40"]
["","","","Vodní okruh – pokles tlaku vody-=-Vytápění-=-45/40&nbsp;°C-=-Max.-=-kPa","kPa","16.30","7.20","8.10"]
["","Chlazení","Vodní okruh – pokles tlaku vody-=-Chlazení-=-7/12&nbsp;°C","Vodní okruh – pokles tlaku vody-=-Chlazení-=-7/12&nbsp;°C-=-Min.-=-kPa","kPa","4.80","4.70","5.50"]
["","","","Vodní okruh – pokles tlaku vody-=-Chlazení-=-7/12&nbsp;°C-=-Stř.-=-kPa","kPa","10.50","5.60","5.40"]
["","","","Vodní okruh – pokles tlaku vody-=-Chlazení-=-7/12&nbsp;°C-=-Max.-=-kPa","kPa","11.70","5.10","5.30"]
["Vodní okruh – průtok vody","Vytápění","Vodní okruh – průtok vody-=-Vytápění-=-45/40&nbsp;°C","Vodní okruh – průtok vody-=-Vytápění-=-45/40&nbsp;°C-=-Min.-=-kg/h","kg/h","100.00","140","150.00"]
["","","","Vodní okruh – průtok vody-=-Vytápění-=-45/40&nbsp;°C-=-Stř.-=-kg/h","kg/h","170.00","240","300.00"]
["","","","Vodní okruh – průtok vody-=-Vytápění-=-45/40&nbsp;°C-=-Max.-=-kg/h","kg/h","260.00","350","420.00"]
["","Chlazení","Vodní okruh – průtok vody-=-Chlazení-=-7/12&nbsp;°C","Vodní okruh – průtok vody-=-Chlazení-=-7/12&nbsp;°C-=-Min.-=-kg/h","kg/h","80.00","110","120.00"]
["","","","Vodní okruh – průtok vody-=-Chlazení-=-7/12&nbsp;°C-=-Stř.-=-kg/h","kg/h","150.00","190","210.00"]
["","","","Vodní okruh – průtok vody-=-Chlazení-=-7/12&nbsp;°C-=-Max.-=-kg/h","kg/h","210.00","280","330.00"]
["Hladina akustického výkonu","Hladina akustického výkonu-=-Min.-=-dBA","","","dBA","35","36","37"]
["","Stř.","","","dBA","46","47","48"]
["","Max.","","","dBA","53.0","54.0","55.0"]
["Provozní rozsah","Vytápění","Vody strana","Min.","°C","30","30","30"]
["","","","Max.","°C","85","85","85"]
["","Chlazení","Vody strana","Min.","°C","5","5","5"]
["","","","Max.","°C","18","18","18"]
["","Vnitřní instalace","Okolí","Min.","°CST","0","0","0"]
["","","","Max.","°CST","45","45","45"]
["Řídicí systémy","Infračervené dálkové ovládání","","","","Pro FWXT-ATV3(C)(CL)","Pro FWXT-ATV3(C)(CL)","Pro FWXT-ATV3(C)(CL)"]
["","Integrace na vnitřní jednotce","","","","Ano","Ano","Ano"]
["Napájení","Fáze","","","","1~","1~","1~"]
["","Frekvence","","","Hz","50","50","50"]
["","Napětí","","","V","230","230","230"]
["Příkon","Max.","","","W","19","20","29"]
["","Režim připravenosti","","","W","3","4","5"]
["Proud","Maximální proud při provozu","","Vytápění","A","0.16","0.18","0.24"]
["","","","Chlazení","A","0.16","0.18","0.24"]