{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":7,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","JEHCCU-CL3"]
[]
[]
[]
[]
["","","","","","JEHCCU0180CL3","JEHCCU0210CL3"]
["Hmotnost","Jednotka","","","kg","80","81"]
["Rozměry","Jednotka","","Šířka","mm","1,101","1,101"]
["","","","Hloubka","mm","444","444"]
["","","","Výška","mm","662","662"]
["Opláštění","Barva","","","","Světle šedá","Světle šedá"]
["Ventilátor","Typ","","","","Axiální","Axiální"]
["Power supply","Fáze","","","","3~","3~"]
["","Frekvence","","","Hz","50","50"]
["","Napětí","","","V","400","400"]
["Poznámky","","","","","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C"]
["","","","","","(2) - Hladina akustického tlaku je měřena v anechoické komoře 10 m","(2) - Hladina akustického tlaku je měřena v anechoické komoře 10 m"]
["","","","","","(3) - Zařízení využívá fluorované skleníkové plyny","(3) - Zařízení využívá fluorované skleníkové plyny"]
["Chladicí výkon","Nízká teplota","R-448A","Jmen.","kW","0.98"]
["","","R-449A","Jmen.","kW","0.98"]
["Vstup napájení","Nízká teplota","R-448A","Jmen.","kW","0.98"]
["","","R-449A","Jmen.","kW","0.98"]
["COP","Nízká teplota","","R-448A","","1.00"]
["","","","R-449A","","1.00"]
["Parametry při plném zatížení při venkovní teplotě 32 °C (Bod A)","R-448A","Te -10 °C","Jmenovitý chladicí výkon (PA)","kW","0.98"]
["","","","Jmenovitý příkon (DA)","kW","0.98"]
["","","","Jmenovité COP (COPA)","","1.00"]
["","R-449A","Te -10 °C","Jmenovitý chladicí výkon (PA)","kW","0.98"]
["","","","Jmenovitý příkon (DA)","kW","0.98"]
["","","","Jmenovité COP (COPA)","","1.00"]
["Parametry při plném zatížení při venkovní teplotě 25 °C","R-448A","Te -35 °C","Deklarované COP (COP2)","","1.15"]
["","","","Příkon (D2)","kW","1.00"]
["","R-449A","Te -35°C","Deklarované COP (COP2)","","1.15"]
["Chladivo","Typ5","","","","R-448A"]
["","GWP Typ 5","","","","1,387"]