{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MC55W"]
[]
[]
[]
[]
["","","","","","MC55WVM"]
["Typ","","","","","Čistička vzduchu"]
["Použití","","","","","Parapetní typ"]
["Opláštění","Colour","","","","Bílý"]
["Rozměry","Jednotka","","Výška","mm","500"]
["","","","Šířka","mm","270"]
["","","","Hloubka","mm","270"]
["Hmotnost","Jednotka","","","kg","6.8"]
["Využitelná plocha místnosti","m²","","","","41 (1), 82 (2)"]
["CADR","m³/h","","","","320"]
["Operace čištění vzduchu","Vstup napájení","","Turbo","kW","0.037"]
["","","","M","kW","0.015"]
["","","","L","kW","0.010"]
["","","","Ticho","kW","0.008"]
["Hladina akustického tlaku","Operace čištění vzduchu","","Turbo","dBA","53"]
["","","","Střední","dBA","39"]
["","","","Nízký","dBA","29"]
["","","","Ticho","dBA","19"]
["Ventilátor","Průtok vzduchu","Operace čištění vzduchu","Turbo","m³/h","330"]
["","","","Střední","m³/h","192"]
["","","","Nízký","m³/h","120"]
["","","","Ticho","m³/h","66"]
["Způsob zachytávání prachu","","","","","Elektrostatický filtr HEPA"]
["Deodorizing method","","","","","Flash streamer + Deodorizační katalyzátor"]
["Bezpečnostní zařízení","Položka","","01","","Safety switch (Operation stops when the Streamer unit cover is open)"]
["Standardní příslušenství","Dálkové ovládání","","","","1"]
["","Držák dálkového ovládání","","","","1"]
["","Elektrostatický filtr HEPA","","","","1"]
["","Deodorizační filtr","","","","1"]
["","Manuální ovládání","","","","1"]
["Napájecí šňůra","m","","","","1.8"]
["Power supply","Phase","","","","1~"]
["","Frekvence","","","Hz","50/60"]
["","Napětí","","","V","220-240/220-230"]
["Proud při provozu","Operace čištění vzduchu","","Turbo","A","0.32"]
["","","","Střední","A","0.14"]
["","","","Nízký","A","0.10"]
["","","","Ticho","A","0.08"]
["Poznámky","","","","","(1) - Použitý prostor místnosti je vhodný pro provoz jednotky při maximálních otáčkách ventilátoru (HH). Využitelná plocha místnosti označuje prostor, ze kterého lze během 30 minut odstranit určité množství prachových částic. (JEM 1467)"]
["","","","","","(2) - Konvertováno ze zkušebních hodnot na normy NRCC podle JEM1467."]
["","","","","","(3) - Konvertováno ze zkušebních hodnot na normy CADR podle JEM1467."]
["","","","","","(4) - Hluk za provozu jsou průměrné hodnoty měřené ve vzdálenosti 1 m od přední, levé, pravé a horní stěny jednotky. (Shodné s hodnotou v anechoické komoře)"]
["","","","","","(5) - Elektrostatický HEPA filtr je vmontován do jednotky."]
["","","","","","(6) - Další funkce: Funkce aktivního odtávání.. Funkce automatického restartu."]