{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MC80Z"]
[]
[]
[]
[]
["","","","","","MC80ZVM"]
["Typ","","","","","Čistička vzduchu"]
["Použití","","","","","Parapetní typ"]
["Opláštění","Barva","","","","Front: White, Top/Side: Dark Grey"]
["Rozměry","Jednotka","","Výška","mm","630"]
["","","","Šířka","mm","315"]
["","","","Hloubka","mm","315"]
["Hmotnost","Jednotka","","","kg","9.8"]
["Využitelná plocha místnosti","m²","","","","62, 124"]
["CADR","m³/h","","","","480"]
["Operace čištění vzduchu","Vstup napájení","","Turbo","kW","0.080"]
["","","","M","kW","0.016"]
["","","","L","kW","0.011"]
["","","","Ticho","kW","0.009"]
["Hladina akustického tlaku","Operace čištění vzduchu","","Turbo","dBA","55"]
["","","","Střední","dBA","34"]
["","","","Nízký","dBA","25"]
["","","","Ticho","dBA","19"]
["Ventilátor","Průtok vzduchu","Operace čištění vzduchu","Turbo","m³/h","480"]
["","","","Střední","m³/h","210"]
["","","","Nízký","m³/h","132"]
["","","","Ticho","m³/h","84"]
["Způsob zachytávání prachu","","","","","Elektrostatický filtr HEPA"]
["Metoda dezodorizace","","","","","Twin streamer + Deodorizační katalyzátor"]
["Standardní příslušenství","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["Napájecí šňůra","m","","","","2"]
["Napájení","Fáze","","","","1~"]
["","Frekvence","","","Hz","50/60"]
["","Napětí","","","V","220-240/220-230"]
["Poznámky","","","","","(1) - Oblast pokrytí je vhodná pro provoz jednotky při maximálních otáčkách ventilátoru (HH). Oblast pokrytí označuje prostor, ze kterého lze během 30 minut odstranit určité množství prachových částic."]
["","","","","","(2) - Konvertováno ze zkušebních hodnot na normy NRCC podle JEM1467."]