{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":6,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK70YV"]
[]
[]
[]
[]
["","","","","","MCK70YVM"]
["Typ","","","","","Zvlhčovací čistička vzduchu"]
["Použití","","","","","Parapetní typ"]
["Opláštění","Barva","","","","Bílá (N9. 0)"]
["Rozměry","Jednotka","","Výška","mm","600 (5)"]
["","","","Šířka","mm","395"]
["","","","Hloubka","mm","287"]
["Hmotnost","Jednotka","","","kg","12.5"]
["Využitelná plocha místnosti","m²","","","","48 (1), 96 (2)"]
["CADR","m³/h","","","","375"]
["Operace čištění vzduchu","Vstup napájení","","Turbo","kW","0.066"]
["","","","M","kW","0.016"]
["","","","L","kW","0.01"]
["","","","Ticho","kW","0.008"]
["Operace zvlhčování","Vstup napájení","","Turbo","kW","0.068"]
["","","","M","kW","0.018"]
["","","","L","kW","0.012"]
["","","","Ticho","kW","0.011"]
["","Objem zásobníku vody","","","l","3.6"]
["Hladina akustického tlaku","Operace čištění vzduchu","","Turbo","dBA","54"]
["","","","Střední","dBA","37"]
["","","","Nízký","dBA","27"]
["","","","Ticho","dBA","18"]
["","Operace zvlhčování","","Turbo","dBA","54"]
["","","","Střední","dBA","37"]
["","","","Nízký","dBA","27"]
["","","","Ticho","dBA","23"]
["Ventilátor","Průtok vzduchu","Operace čištění vzduchu","Turbo","m³/h","420"]
["","","","Střední","m³/h","210"]
["","","","Nízký","m³/h","132"]
["","","","Ticho","m³/h","60"]
["","","Operace zvlhčování","Turbo","m³/h","420"]
["","","","Střední","m³/h","210"]
["","","","Nízký","m³/h","132"]
["","","","Ticho","m³/h","102"]
["Způsob zachytávání prachu","","","","","Elektrostatický filtr HEPA"]
["Metoda dezodorizace","","","","","Flash streamer + Deodorizační katalyzátor"]
["Standardní příslušenství","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","1"]
["Napájecí šňůra","m","","","","2"]
["Napájení","Fáze","","","","1~"]
["","Frekvence","","","Hz","50/60"]
["","Napětí","","","V","220-240/220-230"]
["Poznámky","","","","","(1) - Oblast pokrytí je vhodná pro provoz jednotky při maximálních otáčkách ventilátoru (HH). Oblast pokrytí označuje prostor, ze kterého lze během 30 minut odstranit určité množství prachových částic."]
["","","","","","(2) - Konvertováno ze zkušebních hodnot na normy NRCC podle JEM1467."]
["","","","","","(3) - Hluk za provozu jsou průměrné hodnoty měřené ve vzdálenosti 1 m od přední, levé, pravé a horní stěny jednotky. (Shodné s hodnotou v anechoické komoře)"]