{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":8,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXA-A9"]
[]
[]
[]
[]
["","","","","","RXA20A5V1B9","RXA25A5V1B9","RXA35A5V1B9"]
["Rozměry","Jednotka","","Výška","mm","550","550","550"]
["","","","Šířka","mm","840","840","840"]
["","","","Hloubka","mm","350","350","350"]
["Hmotnost","Jednotka","","","kg","32","32","32"]
["Kompresor","Typ","","","","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor"]
["Provozní rozsah","Chlazení","Okolí","Min.","°CST","-10","-10","-10"]
["","","","Max.","°CST","46","46","46"]
["","Vytápění","Okolí","Min.","° CWB","-15","-15","-15"]
["","","","Max.","° CWB","18","18","18"]
["Hladina akustického tlaku","Chlazení","","Jm.","dBA","46.0","46.0","49.0"]
["","Vytápění","","Jm.","dBA","47.0","47.0","49.0"]
["Chladivo","Typ","","","","R-32","R-32","R-32"]
["","Náplň","","","kg","0.76","0.76","0.76"]
["","Náplň","","","tCO2Eq","0.52","0.52","0.52"]
["","Vliv na globální oteplování (GWP)","","","","675.0","675.0","675.0"]
["Spoje potrubí","Délka potrubí","Max.","OU - IU","m","20","20","20"]
["","Doplňková náplň chladiva","","","kg/m","0,02 (pro délku potrubí přesahující 10m)","0,02 (pro délku potrubí přesahující 10m)","0,02 (pro délku potrubí přesahující 10m)"]
["","Rozdíl hladin","IU - OU","Max.","m","15.0","15.0","15.0"]
["Standardní příslušenství","Příručka pro instalaci","","","","1","1","1"]
["","Štítek náplně chladiva","","","","1","1","1"]
["","Vícejazyčné štítky pro fluorované skleníkové plyny","","","","1","1","1"]
["","Obecná bezpečnostní opatření","","","","1","1","1"]
["","Uzávěr vypouštění","","","","1","1","1"]
["Energetickou účinná řada","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Napájení","Fáze","","","","1~","1~","1~"]
["","Frekvence","","","Hz","50","50","50"]
["","Napětí","","","V","220-240","220-240","220-240"]
["Poznámky","","","","","(1) - Obsahuje fluorované skleníkové plyny","(1) - Obsahuje fluorované skleníkové plyny","(1) - Obsahuje fluorované skleníkové plyny"]
["","","","","","(2) - Viz samostatný výkres s provozním rozsahem","(2) - Viz samostatný výkres s provozním rozsahem","(2) - Viz samostatný výkres s provozním rozsahem"]
["","","","","","(3) - Údaje o elektrickém systému najdete v samostatném výkresu","(3) - Údaje o elektrickém systému najdete v samostatném výkresu","(3) - Údaje o elektrickém systému najdete v samostatném výkresu"]