{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":9,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXA-B"]
[]
[]
[]
[]
["","","","","","RXA42B2V1B","RXA42B5V1B","RXA50B2V1B","RXA50B5V1B"]
["Rozměry","Jednotka","","Výška","mm","734","","734","734"]
["","","","Šířka","mm","870","","870","954"]
["","","","Hloubka","mm","373","","373","401"]
["Hmotnost","Jednotka","","","kg","50","","50","49"]
["Kompresor","Typ","","","","Hermeticky utěsněný rotační kompresor","","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor"]
["Provozní rozsah","Chlazení","Okolí","Min.","°CST","-10","","-10","-10"]
["","","","Max.","°CST","46","","46","46"]
["","Vytápění","Okolí","Min.","° CWB","-15","","-15","-15"]
["","","","Max.","° CWB","18","","18","18"]
["Hladina akustického tlaku","Chlazení","","Jm.","dBA","48.0","","48.0","48"]
["","Vytápění","","Jm.","dBA","48.0","","48.0","48"]
["Chladivo","Typ","","","","R-32","","R-32","R-32"]
["","Náplň","","","kg","1.10","","1.10","1.1"]
["","Náplň","","","tCO2Eq","0.75","","0.75","0.75"]
["","Vliv na globální oteplování (GWP)","","","","675","","675","675"]
["Spoje potrubí","Délka potrubí","Max.","OU - IU","m","30","","30","30"]
["","Doplňková náplň chladiva","","","kg/m","0,02 (pro délku potrubí přesahující 10m)","","0,02 (pro délku potrubí přesahující 10m)","0,02 (pro délku potrubí přesahující 10m)"]
["","Rozdíl hladin","IU - OU","Max.","m","20","","20","20"]
["Standardní příslušenství","Příručka pro instalaci","","","","1","","1","1"]
["","Štítek náplně chladiva","","","","1","","1","1"]
["","Vícejazyčné štítky pro fluorované skleníkové plyny","","","","1","","1","1"]
["","Krytka vypouštění","","","","3","","3","3"]
["","Uzávěr vypouštění","","","","1","","1","1"]
["Energetickou účinná řada","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Napájení","Fáze","","","","1~","","1~","1~"]
["","Frekvence","","","Hz","50","","50","50"]
["","Napětí","","","V","220-240","","220-240","220-240"]
["Poznámky","","","","","(1) - Viz samostatný výkres s provozním rozsahem","","(1) - Viz samostatný výkres s provozním rozsahem","(1) - Viz samostatný výkres s provozním rozsahem"]
["","","","","","(2) - Údaje o elektrickém systému najdete v samostatném výkresu","","(2) - Údaje o elektrickém systému najdete v samostatném výkresu","(2) - Údaje o elektrickém systému najdete v samostatném výkresu"]
["","","","","","(3) - Obsahuje fluorované skleníkové plyny","","(3) - Obsahuje fluorované skleníkové plyny","(3) - Obsahuje fluorované skleníkové plyny"]