{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":11,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXC-D"]
[]
[]
[]
[]
["","","","","","RXC20DV1B","RXC25DV1B","RXC35DV1B","RXC50DV1B","RXC60DV1B","RXC71DV1B"]
["Rozměry","Jednotka","","Výška","mm","550","550","550","615","615","695"]
["","","","Šířka","mm","658","658","658","845","845","930"]
["","","","Hloubka","mm","273","273","273","300","300","350"]
["Hmotnost","Jednotka","","","kg","24.0","24.0","26.0","39.0","39.0","45.0"]
["Kompresor","Typ","","","","Hermetický swing","Hermetický swing","Hermetický swing","Hermetický swing","Hermetický swing","Hermetický swing"]
["Provozní rozsah","Chlazení","Okolí","Min.","°CST","10","10","10","-10","-10","-10"]
["","","","Max.","°CST","46","46","46","46","46","46"]
["","Vytápění","Okolí","Min.","° CWB","-15","-15","-15","-15","-15","-15"]
["","","","Max.","° CWB","18","18","18","18","18","18"]
["Sound power level","Chlazení","","","dBA","58","58","60","65","66","69"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","45","45","46","51","54","54"]
["Chladivo","Typ","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Náplň","","","kg","0.550","0.550","0.750","1.00","1.10","1.15"]
["","Vliv na globální oteplování (GWP)","","","","675.0","675.0","675.0","675.0","675.0","675.0"]
["Spoje potrubí","Doplňková náplň chladiva","","","kg/m","0 017 (pro délku potrubí přesahující 7,5 m)","0 017 (pro délku potrubí přesahující 7,5 m)","0 017 (pro délku potrubí přesahující 7,5 m)","0 017 (pro délku potrubí přesahující 7,5 m)","0 017 (pro délku potrubí přesahující 7,5 m)","0 017 (pro délku potrubí přesahující 7,5 m)"]
["","Rozdíl hladin","IU - OU","Max.","m","15.0","15.0","15.0","20.0","20.0","20.0"]
["Power supply","Fáze","","","","1~","1~","1~","1~","1~","1~"]
["","Frekvence","","","Hz","50","50","50","50","50","50"]
["","Napětí","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]