{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":11,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXC-D"]
[]
[]
[]
[]
["","","","","","RXC20DV1B","RXC25DV1B","RXC35DV1B","RXC50DV1B","RXC60DV1B","RXC71DV1B"]
["Hladina akustického výkonu","Chlazení","","","dBA","58","58","60","65","66","69"]
["Rozměry","Jednotka","","Výška","mm","550","550","550","615","615","695"]
["","","","Šířka","mm","658","658","658","845","845","930"]
["","","","Hloubka","mm","273","273","273","300","300","350"]
["Hmotnost","Jednotka","","","kg","24","24","26","39","39","45"]
["Kompresor","Typ","","","","Hermetický swing","Hermetický swing","Hermetický swing","Hermetický swing","Hermetický swing","Hermetický swing"]
["Provozní rozsah","Chlazení","Okolí","Min.","°CDB","10","10","10","-10","-10","-10"]
["","","","Max.","°CDB","46","46","46","46","46","46"]
["","Vytápění","Okolí","Min.","° CWB","-15","-15","-15","-15","-15","-15"]
["","","","Max.","° CWB","18","18","18","18","18","18"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","45","45","46","51","54","54"]
["Chladivo","Typ","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Náplň","","","kg","0.55","0.55","0.75","1","1.1","1.15"]
["","Náplň","","","tCO2Eq","0.371","0.371","0.506","0.675","0.743","0.776"]
["","Vliv na globální oteplování (GWP)","","","","675.0","675.0","675.0","675.0","675.0","675.0"]
["Spoje potrubí","Délka potrubí","Max.","OU - IU","m","20","20","20","30","30","30"]
["","Doplňková náplň chladiva","","","kg/m","0 017 (pro délku potrubí přesahující 75 m)","0 017 (pro délku potrubí přesahující 75 m)","0 017 (pro délku potrubí přesahující 75 m)","0 017 (pro délku potrubí přesahující 75 m)","0 017 (pro délku potrubí přesahující 75 m)","0 017 (pro délku potrubí přesahující 75 m)"]
["","Rozdíl hladin","IU - OU","Max.","m","15.0","15.0","15.0","20.0","20.0","20.0"]
["Napájení","Fáze","","","","1~","1~","1~","1~","1~","1~"]
["","Frekvence","","","Hz","50","50","50","50","50","50"]
["","Napětí","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]