{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":10,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXF-F"]
[]
[]
[]
[]
["","","","","","RXF20F5V1B (Archived)","RXF25F5V1B (Archived)","RXF35F5V1B (Archived)","RXF42F5V1B (Archived)","RXF50F5V1B (Archived)"]
["Rozměry","Jednotka","","Výška","mm","556","556","556","556","610"]
["","","","Šířka","mm","740","740","740","740","923"]
["","","","Hloubka","mm","343","343","343","343","367"]
["Hmotnost","Jednotka","","","kg","24.0","24.0","24.0","28.0","40.0"]
["Kompresor","Typ","","","","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor"]
["Provozní rozsah","Chlazení","Okolí","Min.","°CST","-10","-10","-10","-10","-10"]
["","","","Max.","°CST","48","48","48","48","48"]
["","Vytápění","Okolí","Min.","° CWB","-15","-15","-15","-15","-15"]
["","","","Max.","° CWB","18","18","18","18","18"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","46.0","46.0","48.0","48.0","48.0"]
["","Vytápění","","Vysoké","dBA","47.0","47.0","48.0","48.0","49.0"]
["Chladivo","Typ","","","","R-32","R-32","R-32","R-32","R-32"]
["","Náplň","","","kg","0.420","0.420","0.500","0.750","0.800"]
["","Náplň","","","tCO2Eq","0.280","0.280","0.340","0.510","0.540"]
["","Vliv na globální oteplování (GWP)","","","","675.0","675.0","675.0","675.0","675.0"]
["Spoje potrubí","Délka potrubí","Max.","OU - IU","m","20","20","20","20","30"]
["","Doplňková náplň chladiva","","","kg/m","002","002","002","002","002"]
["","Rozdíl hladin","IU - OU","Max.","m","12.0","12.0","12.0","12.0","20.0"]
["Standardní příslušenství","Installation manual","","","","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1"]
["","Drain plug","","","","1","1","1","1"]
["Napájení","Fáze","","","","1~","1~","1~","1~","1~"]
["","Frekvence","","","Hz","50","50","50","50","50"]
["","Napětí","","","V","220-240","220-240","220-240","220-240","220-240"]
["Poznámky","","","","","(1) - Obsahuje fluorované skleníkové plyny","(1) - Obsahuje fluorované skleníkové plyny","(1) - Obsahuje fluorované skleníkové plyny","(1) - Obsahuje fluorované skleníkové plyny","(1) - Obsahuje fluorované skleníkové plyny"]
["","","","","","(2) - Údaje o elektrickém systému najdete v samostatném výkresu","(2) - Údaje o elektrickém systému najdete v samostatném výkresu","(2) - Údaje o elektrickém systému najdete v samostatném výkresu","(2) - Údaje o elektrickém systému najdete v samostatném výkresu","(2) - Údaje o elektrickém systému najdete v samostatném výkresu"]
["","","","","","(3) - Viz samostatný výkres s provozním rozsahem","(3) - Viz samostatný výkres s provozním rozsahem","(3) - Viz samostatný výkres s provozním rozsahem","(3) - Viz samostatný výkres s provozním rozsahem","(3) - Viz samostatný výkres s provozním rozsahem"]