{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXLG-M"]
[]
[]
[]
[]
["","","","","","RXLG25M2V1B","RXLG35M2V1B"]
["Ventilátor","Průtok vzduchu","Chlazení","Velmi nízké","m³/min","30.6","30.6"]
["","","Vytápění","Velmi nízké","m³/min","27.2","27.2"]
["","","","Velmi nízké","cfm","1080","1080"]
["","","Vytápění","Velmi nízké","cfm","960","960"]
["Rozměry","Jednotka","","Výška","mm","550","550"]
["","","","Šířka","mm","858","858"]
["","","","Hloubka","mm","330","330"]
["Hmotnost","Jednotka","","","kg","40","40"]
["Kompresor","Typ","","","","","Hermeticky utěsněný rotační kompresor"]
["Provozní rozsah","Chlazení","Okolí","Min.","°CDB","-10","-10"]
["","","","Max.","°CDB","46","46"]
["","Vytápění","Okolí","Min.","° CWB","-25","-25"]
["","","","Max.","° CWB","18","18"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","48","48"]
["","","","Nízký","dBA","44","44"]
["","Vytápění","","Vysoké","dBA","49","49"]
["","","","Nízký","dBA","45","45"]
["Chladivo","Typ","","","","R-410A","R-410A"]
["","Náplň","","","kg","1","1"]
["","Náplň","","","tCO2Eq","2.1","2.1"]
["","Vliv na globální oteplování (GWP)","","","","2087.5","2087.5"]
["Spoje potrubí","Délka potrubí","Max.","OU - IU","m","20","20"]
["","Doplňková náplň chladiva","","","kg/m","0,02 (pro délku potrubí přesahující 10m)","0,02 (pro délku potrubí přesahující 10m)"]
["","Rozdíl hladin","IU - IU","Max.","m","15","15"]
["Standardní příslušenství","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["Napájení","Fáze","","","","1~","1~"]
["","Frekvence","","","Hz","50","50"]
["","Napětí","","","V","220-240","220-240"]
["Kompresor","Typ","","","","Hermeticky utěsněný rotační kompresor"]