{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":12,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-A"]
[]
[]
[]
[]
["","","","","","RXM20A5V1B","RXM25A5V1B","RXM35A5V1B","RXM42A5V1B","RXM50A5V1B","RXM60A5V1B","RXM71A5V1B"]
["Rozměry","Jednotka","","Výška","mm","610","610","610","610","734","734","734"]
["","","","Šířka","mm","923","923","923","923","954","954","954"]
["","","","Hloubka","mm","367","367","367","367","401","401","401"]
["Hmotnost","Jednotka","","","kg","36","36","36","40","49","49","55"]
["Motor ventilátoru","Otáčky","Chlazení","Velmi nízké","ot./min","600","600","600","600","500"]
["Kompresor","Typ","","","","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor"]
["Provozní rozsah","Chlazení","Okolí","Min.","°CST","-10","-10","-10","-10","-10","-10","-10"]
["","","","Max.","°CST","50","50","50","50","50 (1)","50","46"]
["","Vytápění","Okolí","Min.","° CWB","-21","-21","-21","-21","-21 (1)","-21","-15"]
["","","","Max.","° CWB","18","18","18","18","18","18","18"]
["Hladina akustického tlaku","Chlazení","","Jm.","dBA","46","46","47","48","48","48","47"]
["","Vytápění","","Jm.","dBA","47","47","49","49","49","49","48"]
["Chladivo","Typ","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Náplň","","","kg","0.95","0.95","0.95","0.95","1.10","1.15","1.15"]
["","Náplň","","","tCO2Eq","0.65","0.65","0.65","0.65","0.75","0.78","0.78"]
["","Vliv na globální oteplování (GWP)","","","","675","675","675","675","675","675","675"]
["Spoje potrubí","Délka potrubí","Max.","OU - IU","m","20","20","20","30","30","30","30"]
["","Doplňková náplň chladiva","","","kg/m","0,02 (pro délku potrubí přesahující 10m)","0,02 (pro délku potrubí přesahující 10m)","0,02 (pro délku potrubí přesahující 10m)","0,02 (pro délku potrubí přesahující 10m)","0,02 (pro délku potrubí přesahující 10m)","0,02 (pro délku potrubí přesahující 10m)","0,02 (pro délku potrubí přesahující 10m)"]
["","Rozdíl hladin","IU - OU","Max.","m","15","15","15","20","20","20","20"]
["Napájení","Fáze","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Frekvence","","","Hz","50","50","50","50","50","50","50"]
["","Napětí","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Standardní příslušenství","Installation manual","","","","1","1","1","1","1","1","1"]
["","Drain joint","","","","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1","1","1"]
["","Drain cap","","","","3","3","3","3","1","3","3"]
["Poznámky","","","","","","","","","(1) - Viz samostatný výkres s provozním rozsahem","(1) - Viz samostatný výkres s provozním rozsahem","(1) - Viz samostatný výkres s provozním rozsahem"]
["","","","","","","","","","(2) - Údaje o elektrickém systému najdete v samostatném výkresu","(2) - Údaje o elektrickém systému najdete v samostatném výkresu","(2) - Údaje o elektrickém systému najdete v samostatném výkresu"]
["","","","","","","","","","(3) - Obsahuje fluorované skleníkové plyny","(3) - Obsahuje fluorované skleníkové plyny","(3) - Obsahuje fluorované skleníkové plyny"]
["Standardní příslušenství","Drain plug","","","","","","","","","1","1"]