{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":8,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-A9"]
[]
[]
[]
[]
["","","","","","RXM25A5V1B9","RXM35A5V1B9","RXM50A5V1B9"]
["Rozměry","Jednotka","","Výška","mm","610","610","734"]
["","","","Šířka","mm","923","923","954"]
["","","","Hloubka","mm","367","367","401"]
["Hmotnost","Jednotka","","","kg","36","36","49"]
["Motor ventilátoru","Otáčky","Chlazení","Velmi nízké","ot./min","600","600","500"]
["Kompresor","Typ","","","","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor"]
["Provozní rozsah","Chlazení","Okolí","Min.","°CST","-10","-10","-10"]
["","","","Max.","°CST","50","50","46 (1)"]
["","Vytápění","Okolí","Min.","° CWB","-21","-21","-15 (1)"]
["","","","Max.","° CWB","18","18","18"]
["Hladina akustického tlaku","Chlazení","","Jm.","dBA","46","47","48"]
["","Vytápění","","Jm.","dBA","47","49","49"]
["Chladivo","Typ","","","","R-32","R-32","R-32"]
["","Náplň","","","kg","0.95","0.95","1.10"]
["","Náplň","","","tCO2Eq","0.65","0.65","0.75"]
["","Vliv na globální oteplování (GWP)","","","","675","675","675"]
["Spoje potrubí","Délka potrubí","Max.","OU - IU","m","20","20","30"]
["","Doplňková náplň chladiva","","","kg/m","0,02 (pro délku potrubí přesahující 10m)","0,02 (pro délku potrubí přesahující 10m)","0,02 (pro délku potrubí přesahující 10m)"]
["","Rozdíl hladin","IU - OU","Max.","m","15","15","20"]
["Standardní příslušenství","RXM25A5V1B9","","","","1"]
["","Installation manual","","","","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Drain cap","","","","3","3","1"]
["Napájení","Fáze","","","","1~","1~","1~"]
["","Frekvence","","","Hz","50","50","50"]
["","Napětí","","","V","220-240","220-240","220-240"]
["Poznámky","","","","","(1) - Viz samostatný výkres s provozním rozsahem","(1) - Viz samostatný výkres s provozním rozsahem","(1) - Viz samostatný výkres s provozním rozsahem"]
["","","","","","(2) - Údaje o elektrickém systému najdete v samostatném výkresu","(2) - Údaje o elektrickém systému najdete v samostatném výkresu","(2) - Údaje o elektrickém systému najdete v samostatném výkresu"]
["","","","","","(3) - Obsahuje fluorované skleníkové plyny","(3) - Obsahuje fluorované skleníkové plyny","(3) - Obsahuje fluorované skleníkové plyny"]
["Standardní příslušenství","RXM35A5V1B9","","","","","1"]