{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":14,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-N9"]
[]
[]
[]
[]
["","","","","","RXM20N5V1B9","RXM20N2V1B9","RXM25N2V1B9","RXM25N5V1B9","RXM35N2V1B9","RXM35N5V1B9","RXM42N2V1B9","RXM50N2V1B9","RXM60N2V1B9"]
["Rozměry","Jednotka","","Výška","mm","550","550","550","550","550","550","734","734","734"]
["","","","Šířka","mm","765","765","765","765","765","765","870","870","870"]
["","","","Hloubka","mm","285","285","285","285","285","285","373","373","373"]
["Hmotnost","Jednotka","","","kg","32","32","32","32","32","32","50","50","50"]
["Kompresor","Type","","","","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor","","","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor","","","Hermeticky utěsněný rotační kompresor"]
["Provozní rozsah","Chlazení","Okolí","Min.","°CST","-10, -10","-10, -10","-10 (4) (5), -10 (4) (5)","-10 (4) (5), -10 (4) (5)","-10, -10","-10, -10","-10 (5) (4), -10 (5) (4)","-10 (5) (4), -10 (5) (4)","-10, -10"]
["","","","Max.","°CST","50, 46","50, 46","50 (4), 46 (5)","50 (4), 46 (5)","50, 46","50, 46","50 (4), 46 (5)","50 (4), 46 (5)","50, 46"]
["Hladina akustického tlaku","Chlazení","","Jm.","dBA","46","46","46","46","49","49","48","48","48"]
["","Vytápění","","Jm.","dBA","47","47","47","47","49","49","48","49","49"]
["Chladivo","Typ","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Náplň","","","kg","0.76","0.76","0.76","0.76","0.76","0.76","1.10","1.15","1.15"]
["","Náplň","","","tCO2Eq","0.52","0.52","0.52","0.52","0.52","0.52","0.75","0.78","0.78"]
["","Vliv na globální oteplování (GWP)","","","","675","675","675","675","675","675","675","675","675"]
["Spoje potrubí","Délka potrubí","Max.","OU - IU","m","20","20","20","20","20","20","30","30","30"]
["","Doplňková náplň chladiva","","","kg/m","0,02 (pro délku potrubí přesahující 10m)","0,02 (pro délku potrubí přesahující 10m)","0,02 (pro délku potrubí přesahující 10m)","0,02 (pro délku potrubí přesahující 10m)","0,02 (pro délku potrubí přesahující 10m)","0,02 (pro délku potrubí přesahující 10m)","0,02 (pro délku potrubí přesahující 10m)","0,02 (pro délku potrubí přesahující 10m)","0,02 (pro délku potrubí přesahující 10m)"]
["","Rozdíl hladin","IU - OU","Max.","m","15","15","15","15","15","15","20","20","20"]
["Standardní příslušenství","Installation manual","","","","1","1","1","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1","1","1","1"]
["","Drain plug","","","","1","1","1","1","1","1","1","1","1"]
["Napájení","Fáze","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Frekvence","","","Hz","50","50","50","50","50","50","50","50","50"]
["","Napětí","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Poznámky","","","","","(1) - Možné pouze v kombinaci s CTXM*N2V1B, ATXM*N2V1B, FTXM*N2V1B","(1) - Možné pouze v kombinaci s CTXM*N2V1B, ATXM*N2V1B, FTXM*N2V1B","(1) - Možné pouze v kombinaci s CTXM*N2V1B, ATXM*N2V1B, FTXM*N2V1B","(1) - Možné pouze v kombinaci s CTXM*N2V1B, ATXM*N2V1B, FTXM*N2V1B","(1) - Možné pouze v kombinaci s CTXM*N2V1B, ATXM*N2V1B, FTXM*N2V1B","(1) - Možné pouze v kombinaci s CTXM*N2V1B, ATXM*N2V1B, FTXM*N2V1B","(1) - Možné pouze v kombinaci s CTXM*N2V1B, ATXM*N2V1B, FTXM*N2V1B","(1) - Možné pouze v kombinaci s CTXM*N2V1B, ATXM*N2V1B, FTXM*N2V1B","(1) - Možné pouze v kombinaci s CTXM*N2V1B, ATXM*N2V1B, FTXM*N2V1B"]
["","","","","","(2) - Možné pouze v kombinaci s CTXM*M2V1B, ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9, FDXM*F3V1B9, FNA*A2VEB9","(2) - Možné pouze v kombinaci s CTXM*M2V1B, ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9, FDXM*F3V1B9, FNA*A2VEB9","(2) - Možné pouze v kombinaci s CTXM*M2V1B, ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9, FDXM*F3V1B9, FNA*A2VEB9","(2) - Možné pouze v kombinaci s CTXM*M2V1B, ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9, FDXM*F3V1B9, FNA*A2VEB9","(2) - Možné pouze v kombinaci s CTXM*M2V1B, ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9, FDXM*F3V1B9, FNA*A2VEB9","(2) - Možné pouze v kombinaci s CTXM*M2V1B, ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9, FDXM*F3V1B9, FNA*A2VEB9","(2) - Možné pouze v kombinaci s CTXM*M2V1B, ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9, FDXM*F3V1B9, FNA*A2VEB9","(2) - Možné pouze v kombinaci s CTXM*M2V1B, ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9, FDXM*F3V1B9, FNA*A2VEB9","(2) - Možné pouze v kombinaci s CTXM*M2V1B, ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9, FDXM*F3V1B9, FNA*A2VEB9"]
["Kompresor","Typ","","","","","","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor","","","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor"]
["Standardní příslušenství","Drain cap","","","","","","","","","","3","3","3"]