{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F"]
[]
[]
[]
[]
["","","","","","RXS60F4V1B","RXS60F2V1B","RXS60F3V1B","RXS71FAV1B9","RXS71FV1B","RXS71FAV1B"]
["Hladina akustického tlaku","Vytápění","","Vysoké","dBA","49","","","52"]
["","","","Nízký","dBA","46","","","49"]
["","Chlazení","","Nízký","dBA","46","","","49"]
["","","","Vysoké","dBA","49","","","52"]
["Standardní příslušenství","Vypouštěcí hrdlo","","","","1","","","1"]
["","Příručka pro instalaci","","","","1","","","1"]
["Chladivo","Charge","","","TCO2Eq","3.1","","","4.8"]
["","Vliv na globální oteplování (GWP)","","","","2,087.5","","","2,087.5"]
["","Náplň","","","kg","1.5","","","2.3"]
["","Type","","","","R-410A","","","R-410A"]
["Spoje potrubí","Rozdíl hladin","IU - OU","Max.","m","20","","","20"]
["","Doplňková náplň chladiva","","","kg/m","0,02 (pro délku potrubí přesahující 10m)","","","0,02 (pro délku potrubí přesahující 10m)"]
["Kompresor","Typ","","","","Hermeticky utěsněný rotační kompresor","","","Hermeticky utěsněný rotační kompresor"]
["Rozměry","Unit","","Width","mm","825","","","900"]
["","","","Depth","mm","300","","","320"]
["","","","Height","mm","735","","","770"]
["Hmotnost","Unit","","","kg","48","","","71"]
["Power supply","Fáze","","","","1~","","","1~"]
["","Frekvence","","","Hz","50","","","50"]
["","Napětí","","","V","220-240","","","220-240"]
["Poznámky","","","","","(1) - SL: Luftstrømmens hastighedsindstillings lydløse ventilatorniveau","(1) - 220 V","","(1) - SL: Luftstrømmens hastighedsindstillings lydløse ventilatorniveau","(1) - 220 V"]
["","","","","","(2) - Obsahuje fluorované skleníkové plyny","(2) - 230V","","(2) - Obsahuje fluorované skleníkové plyny","(2) - 230V"]
["Rozměry","Jednotka","","Výška","mm","","735","735","","770","770"]
["","","","Šířka","mm","","825","825","","900","900"]
["","","","Hloubka","mm","","300","300","","320","320"]
["Hmotnost","Jednotka","","","kg","","48","48","","71","71"]
["Kompresor","Typ","","","","","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor","","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor"]
["Provozní rozsah","Chlazení","Okolí","Min.","°CDB","","-10","-10","","-10","-10"]
["","","","Max.","°CDB","","46","46","","46","46"]
["","Vytápění","Okolí","Min.","° CWB","","-15","-15","","-15","-15"]
["","","","Max.","° CWB","","18","20","","18","20"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","","49","49","","52","52"]
["","","","Nízký","dBA","","46","46","","49","49"]
["","Vytápění","","Vysoké","dBA","","49","49","","52","52"]
["","","","Nízký","dBA","","46","46","","49","49"]
["Chladivo","Typ","","","","","R-410A","R-410A","","R-410A","R-410A"]
["","Náplň","","","kg","","1.5","1.5","","2.3","2.3"]
["","Náplň","","","tCO2Eq","","3.1","3.1","","4.8","4.8"]
["","Vliv na globální oteplování (GWP)","","","","","2087.5","2087.5","","2087.5","2087.5"]
["Spoje potrubí","Délka potrubí","Max.","OU - IU","m","","30","30","","30","30"]
["","Doplňková náplň chladiva","","","kg/m","","0,02 (pro délku potrubí přesahující 10m)","0,02 (pro délku potrubí přesahující 10m)","","0,02 (pro délku potrubí přesahující 10m)","0,02 (pro délku potrubí přesahující 10m)"]
["","Rozdíl hladin","IU - OU","Max.","m","","20","20","","20","20"]
["Standardní příslušenství","Installation manual","","","","","Installation manual","1","","Installation manual","1"]
["","Drain plug","","","","","Drain plug","","","Drain plug"]
["Napájení","Fáze","","","","","1~","1~","","1~","1~"]
["","Frekvence","","","Hz","","50","50","","50","50"]
["","Napětí","","","V","","220-240","220-240","","220-240","220-240"]
["Poznámky","","","","","","(3) - 240 V","","","(3) - 240 V"]
["Standardní příslušenství","Drain socket","","","","","","1","","","1"]
["Hladina akustického výkonu","Chlazení","","","dBA","","","","65"]