{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":6,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F8"]
[]
[]
[]
[]
["","","","","","RXS71FAV1B8"]
["Ventilátor","Průtok vzduchu","Chlazení","Velmi nízké","m³/min","46.0"]
["","","Vytápění","Velmi nízké","m³/min","46.0"]
["","","","Velmi nízké","cfm","1624"]
["","","Vytápění","Velmi nízké","cfm","1624"]
["Rozměry","Jednotka","","Výška","mm","770"]
["","","","Šířka","mm","900"]
["","","","Hloubka","mm","320"]
["Hmotnost","Jednotka","","","kg","71"]
["Motor ventilátoru","Otáčky","Chlazení","Velmi nízké","ot./min","730"]
["","","Vytápění","Velmi nízké","ot./min","730"]
["Kompresor","Typ","","","","Hermeticky utěsněný rotační kompresor"]
["Provozní rozsah","Chlazení","Okolí","Min.","°CDB","-10"]
["","","","Max.","°CDB","46"]
["","Vytápění","Okolí","Min.","° CWB","-15"]
["","","","Max.","° CWB","18"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","52"]
["","Vytápění","","Vysoké","dBA","52"]
["Chladivo","Typ","","","","R-410A"]
["","Náplň","","","kg","2.3"]
["","Náplň","","","tCO2Eq","4.8"]
["","Vliv na globální oteplování (GWP)","","","","2087.5"]
["Spoje potrubí","Délka potrubí","Max.","OU - IU","m","30"]
["","Doplňková náplň chladiva","","","kg/m","0,02 (pro délku potrubí přesahující 10m)"]
["","Rozdíl hladin","IU - OU","Max.","m","20"]
["Standardní příslušenství","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain socket assy","","","","1"]
["Napájení","Fáze","","","","1~"]
["","Frekvence","","","Hz","50"]
["","Napětí","","","V","220-240"]
["Poznámky","","","","","(1) - 220 V"]
["","","","","","(2) - 230V"]
["","","","","","(3) - 240 V"]