{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":12,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-K"]
[]
[]
[]
[]
["","","","","","RXS20K3V1B","RXS20K2V1B","RXS25K3V1B","RXS25K2V1B","RXS35K2V1B","RXS42K2V1B","RXS50K2V1B"]
["Hladina akustického tlaku","Vytápění","","Vysoké","dBA","47","","47","","48","48","48"]
["","Chlazení","","Vysoké","dBA","46","","46","","48","48","48"]
["Standardní příslušenství","Spoj (odtok)","","","","1","","1"]
["","Příručka pro instalaci","","","","1","","1","","1","1","1"]
["Chladivo","Charge","","","TCO2Eq","2.1","","2.1","","2.5","2.7","3.5"]
["","Vliv na globální oteplování (GWP)","","","","2,087.5","","2,087.5","","2,087.5","2,087.5","2,087.5"]
["","Náplň","","","kg","1.0","","1.0","","1.2","1.3","1.7"]
["","Typ","","","","R-410A","","R-410A","","R-410A","R-410A","R-410A"]
["Motor ventilátoru","Otáčky","Chlazení","Velmi nízké","ot./min","780","","780","","780","790","670"]
["","","Vytápění","Velmi nízké","ot./min","740","","740","","740","780","670"]
["Spoje potrubí","Rozdíl hladin","IU - OU","Max.","m","15","","15","","15","15","20"]
["","Doplňková náplň chladiva","","","kg/m","0,02 (pro délku potrubí přesahující 10m)","","0,02 (pro délku potrubí přesahující 10m)","","0,02 (pro délku potrubí přesahující 10m)","0,02 (pro délku potrubí přesahující 10m)","0,02 (pro délku potrubí přesahující 10m)"]
["Kompresor","Typ","","","","Hermeticky utěsněný rotační kompresor","","Hermeticky utěsněný rotační kompresor","","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor"]
["Rozměry","Jednotka","","Šířka","mm","765","","765","","765","765","825"]
["","","","Hloubka","mm","285","","285","","285","285","300"]
["","","","Výška","mm","550","","550","","550","550","735"]
["Hmotnost","Jednotka","","","kg","34","","34","","34","39","47"]
["Ventilátor","Průtok vzduchu","Vytápění","Velmi nízké","cfm","","","","","904","960","1,522"]
["","","Chlazení","Velmi nízké","cfm","","","","","1,063","1,080","1,727"]
["Power supply","Fáze","","","","1~","","1~","","1~","1~","1~"]
["","Frekvence","","","Hz","50","","50","","50","50","50"]
["","Napětí","","","V","220-240","","220-240","","220-240","220-240","220-240"]
["Poznámky","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V"]
["","","","","","(4) - SL: Luftstrømmens hastighedsindstillings lydløse ventilatorniveau","","(4) - SL: Luftstrømmens hastighedsindstillings lydløse ventilatorniveau","","(4) - Obsahuje fluorované skleníkové plyny","(4) - Obsahuje fluorované skleníkové plyny","(4) - Obsahuje fluorované skleníkové plyny"]
["","","","","","(5) - Obsahuje fluorované skleníkové plyny","","(5) - Obsahuje fluorované skleníkové plyny"]
["Rozměry","Jednotka","","Výška","mm","","550","","550"]
["","","","Šířka","mm","","765","","765"]
["","","","Hloubka","mm","","285","","285"]
["Hmotnost","Jednotka","","","kg","","34","","34"]
["Motor ventilátoru","Otáčky","Chlazení","Velmi nízké","ot./min","","780","","780"]
["","","Vytápění","Velmi nízké","ot./min","","740","","740"]
["Kompresor","Typ","","","","","Hermeticky utěsněný rotační kompresor","","Hermeticky utěsněný rotační kompresor"]
["Provozní rozsah","Chlazení","Okolí","Min.","°CST","","-10","","-10"]
["","","","Max.","°CST","","46","","46"]
["","Vytápění","Okolí","Min.","° CWB","","-15","","-15"]
["","","","Max.","° CWB","","18","","18"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","","46","","46"]
["","Vytápění","","Vysoké","dBA","","47","","47"]
["Chladivo","Typ","","","","","R-410A","","R-410A"]
["","Náplň","","","kg","","1.0","","1.0"]
["","Náplň","","","tCO2Eq","","2.1","","2.1"]
["","Vliv na globální oteplování (GWP)","","","","","2087.5","","2087.5"]
["Spoje potrubí","Délka potrubí","Max.","OU - IU","m","","20","","20"]
["","Doplňková náplň chladiva","","","kg/m","","0,02 (pro délku potrubí přesahující 10m)","","0,02 (pro délku potrubí přesahující 10m)"]
["","Rozdíl hladin","IU - OU","Max.","m","","15","","15"]
["Standardní příslušenství","Installation manual","","","","","1","","1"]
["","Joint (drain)","","","","","1","","1"]
["Napájení","Fáze","","","","","1~","","1~"]
["","Frekvence","","","Hz","","50","","50"]
["","Napětí","","","V","","220-240","","220-240"]
["Standardní příslušenství","Uzávěr vypouštění","","","","","","","","1","1","1"]