{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":73,"n_cols":11,"rows_kept":73,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L"]
[]
[]
[]
[]
["","","","","","RXS20L2V1B","RXS25L2V1B","RXS35L2V1B","RXS42L2V1B","RXS50L2V1B","RXS60L2V1B"]
["Hladina akustického tlaku","Vytápění","","Vysoké","dBA","47","47","48","48"]
["","Chlazení","","Vysoké","dBA","46","46","48","48"]
["Standardní příslušenství","Krytka vypouštění","","","","1","1","","1"]
["","Příručka pro instalaci","","","","1","1","1","1"]
["","Štítek náplně chladiva","","","","1","1","1"]
["","Vícejazyčné štítky pro fluorované skleníkové plyny","","","","1","1","Vícejazyčné štítky pro fluorované skleníkové plyny"]
["Chladivo","Charge","","","TCO2Eq","2.1","2.1","2.5","2.7"]
["","Vliv na globální oteplování (GWP)","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Náplň","","","kg","1.0","1.0","1.20","1.3"]
["","Typ","","","","R-410A","R-410A","R-410A","R-410A"]
["Motor ventilátoru","Otáčky","Chlazení","Velmi nízké","ot./min","780","780","780","790"]
["","","Vytápění","Velmi nízké","ot./min","740","740","740","780"]
["Provozní rozsah","Chlazení","Okolí","Max.","°CST","46","46","46","46"]
["","","","Min.","°CST","-10","-10","-10","-10"]
["","Vytápění","Okolí","Max.","° CWB","18","18","18","18"]
["","","","Min.","° CWB","-15","-15","-15","-15"]
["Připojovací rozměry","Rozdíl hladin","IU - OU","Max.","m","","","15"]
["","Doplňková náplň chladiva","","","kg/m","","","0,020 (pro délku potrubí přesahující 10m)"]
["Rozměry","Jednotka","","Šířka","mm","765","765","765","765"]
["","","","Hloubka","mm","285","285","285","285"]
["","","","Výška","mm","550","550","550","550"]
["Kompresor","Typ","","","","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor"]
["Hmotnost","Jednotka","","","kg","34","34","34","39"]
["Ventilátor","Průtok vzduchu","Vytápění","Velmi nízké","cfm","904","904","904","960"]
["","","","Velmi nízké","m³/min","25.6","25.6","25.6","27.2"]
["","","Chlazení","Velmi nízké","m³/min","30.1","30.1","30.1","30.6"]
["","","","Velmi nízké","cfm","1,063","1,063","1,063","1,080"]
["Power supply","Fáze","","","","1~","1~","1~","1~"]
["","Frekvence","","","Hz","50","50","50","50"]
["","Napětí","","","V","220-240","220-240","220-240","220-240"]
["Poznámky","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V"]
["","","","","","(4) - Obsahuje fluorované skleníkové plyny","(4) - Obsahuje fluorované skleníkové plyny","(4) - Obsahuje fluorované skleníkové plyny","(4) - Obsahuje fluorované skleníkové plyny"]
["Standardní příslušenství","Uzávěr vypouštění","","","","","","1"]
["Ventilátor","Průtok vzduchu","Chlazení","Velmi nízké","m³/min","","","","","48.9","45.0"]
["","","Vytápění","Velmi nízké","m³/min","","","","","43.1","46.3"]
["","","","Velmi nízké","cfm","","","","","1727","1589"]
["","","Vytápění","Velmi nízké","cfm","","","","","1522","1635"]
["Rozměry","Jednotka","","Výška","mm","","","","","735","735"]
["","","","Šířka","mm","","","","","825","825"]
["","","","Hloubka","mm","","","","","300","300"]
["Hmotnost","Jednotka","","","kg","","","","","47","48"]
["Motor ventilátoru","Otáčky","Chlazení","Velmi nízké","ot./min","","","","","670"]
["","","Vytápění","Velmi nízké","ot./min","","","","","670"]
["Kompresor","Typ","","","","","","","","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor"]
["Provozní rozsah","Chlazení","Okolí","Min.","°CST","","","","","-10","-10"]
["","","","Max.","°CST","","","","","46","46"]
["","Vytápění","Okolí","Min.","° CWB","","","","","-15","-15"]
["","","","Max.","° CWB","","","","","18","18"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","","","","","48","49"]
["","","","Nízký","dBA","","","","","44","46"]
["","Vytápění","","Vysoké","dBA","","","","","48","49"]
["","","","Nízký","dBA","","","","","45","46"]
["Chladivo","Typ","","","","","","","","R-410A","R-410A"]
["","Náplň","","","kg","","","","","1.7","1.5"]
["","Náplň","","","tCO2Eq","","","","","3.5","3.1"]
["","Vliv na globální oteplování (GWP)","","","","","","","","2087.5","2087.5"]
["Spoje potrubí","Délka potrubí","Max.","OU - IU","m","","","","","30","30"]
["","Doplňková náplň chladiva","","","kg/m","","","","","0,020 (pro délku potrubí přesahující 10m)","0,020 (pro délku potrubí přesahující 10m)"]
["","Rozdíl hladin","IU - OU","Max.","m","","","","","20.0","20"]
["Standardní příslušenství","Installation manual","","","","","","","","1","1"]
["","Drain plug","","","","","","","","1","1"]
["Napájení","Fáze","","","","","","","","1~","1~"]
["","Frekvence","","","Hz","","","","","50","50"]
["","Napětí","","","V","","","","","220-230-240","220-230-240"]
["Poznámky","","","","","","","","","","(1) - 230V"]