{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":72,"n_cols":8,"rows_kept":72,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L3"]
[]
[]
[]
[]
["","","","","","RXS20L3V1B","RXS25L3V1B","RXS35L3V1B"]
["Hladina akustického tlaku","Vytápění","","Vysoké","dBA","","","48"]
["","Chlazení","","Vysoké","dBA","","","48"]
["Standardní příslušenství","Příručka pro instalaci","","","","","","1"]
["","Štítek náplně chladiva","","","","","","1"]
["","Vícejazyčné štítky pro fluorované skleníkové plyny","","","","","","1"]
["","Vypouštěcí zátka (pouze modely tepelných čerpadel)","","","","","","1"]
["Chladivo","Charge","","","TCO2Eq","","","2.5"]
["","GWP","","","","","","2,087.5"]
["","Náplň","","","kg","","","1.2"]
["","Type","","","","","","R-410A"]
["Motor ventilátoru","Otáčky","Chlazení","Velmi nízké","ot./min","","","780"]
["","","Vytápění","Velmi nízké","ot./min","","","740"]
["Provozní rozsah","Chlazení","Okolí","Max.","°CST","","","46"]
["","","","Min.","°CST","","","-10"]
["","Vytápění","Okolí","Max.","° CWB","","","18"]
["","","","Min.","° CWB","","","-15"]
["Spoje potrubí","Rozdíl hladin","IU - OU","Max.","m","","","15"]
["","Doplňková náplň chladiva","","","kg/m","","","0,02 (pro délku potrubí přesahující 10m)"]
["Rozměry","Jednotka","","Šířka","mm","","","765"]
["","","","Hloubka","mm","","","285"]
["","","","Výška","mm","","","550"]
["Kompresor","Typ","","","","","","Hermeticky utěsněný rotační kompresor"]
["Hmotnost","Jednotka","","","kg","","","34"]
["Fan","Průtok vzduchu","Vytápění","Velmi nízké","cfm","","","904"]
["","","","Velmi nízké","m³/min","","","25.6"]
["","","Chlazení","Velmi nízké","m³/min","","","30.1"]
["","","","Velmi nízké","cfm","","","1,063"]
["Power supply","Fáze","","","","","","1~"]
["","Frekvence","","","Hz","","","50"]
["","Napětí","","","V","","","220-240"]
["Poznámky","","","","","","","(1) - SL: Luftstrømmens hastighedsindstillings lydløse ventilatorniveau"]
["Ventilátor","Průtok vzduchu","Chlazení","Velmi nízké","m³/min","30.1","30.1"]
["","","Vytápění","Velmi nízké","m³/min","25.6","25.6"]
["","","","Velmi nízké","cfm","1063","1063"]
["","","Vytápění","Velmi nízké","cfm","904","904"]
["Rozměry","Jednotka","","Výška","mm","550","550"]
["","","","Šířka","mm","765","765"]
["","","","Hloubka","mm","285","285"]
["Hmotnost","Jednotka","","","kg","34","34"]
["Motor ventilátoru","Otáčky","Chlazení","Velmi nízké","ot./min","780","780"]
["","","Vytápění","Velmi nízké","ot./min","740","740"]
["Kompresor","Typ","","","","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor"]
["Provozní rozsah","Chlazení","Okolí","Min.","°CST","-10","-10"]
["","","","Max.","°CST","46","46"]
["","Vytápění","Okolí","Min.","° CWB","-15","-15"]
["","","","Max.","° CWB","18","18"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","46","46"]
["","Vytápění","","Vysoké","dBA","47","47"]
["Chladivo","Typ","","","","R-410A","R-410A"]
["","Náplň","","","kg","1.0","1.0"]
["","Náplň","","","tCO2Eq","2.1","2.1"]
["","Vliv na globální oteplování (GWP)","","","","2087.5","2087.5"]
["Spoje potrubí","Délka potrubí","Max.","OU - IU","m","20","20"]
["","Doplňková náplň chladiva","","","kg/m","0,02 (pro délku potrubí přesahující 10m)","0,02 (pro délku potrubí přesahující 10m)"]
["","Rozdíl hladin","IU - OU","Max.","m","15","15"]
["Standardní příslušenství","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["","Drain plug","","","","1"]
["Napájení","Fáze","","","","1~","1~"]
["","Frekvence","","","Hz","50","50"]
["","Napětí","","","V","220-240","220-240"]
["Poznámky","","","","","(1) - 220 V"]
["","","","","","(2) - 230V"]
["","","","","","(3) - 240 V"]
["Standardní příslušenství","Drain plug (only heat pump models)","","","","","1"]