{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":11,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXZ-N"]
[]
[]
[]
[]
["","","","","","RXZ25NV1B","RXZ25NV1B9","RXZ35NV1B","RXZ35NV1B9","RXZ50NV1B","RXZ50NV1B9"]
["Hladina akustického tlaku","Vytápění","","Vysoké","dBA","","","48","48","50","50"]
["","Chlazení","","Vysoké","dBA","","","48","48","49","49"]
["Standardní příslušenství","Manuální ovládání","","","","","","1","1","1","1"]
["","Příručka pro instalaci","","","","","","1","1","1","1"]
["Chladivo","Vliv na globální oteplování (GWP)","","","","","","675","675","675","675"]
["","Náplň","","","kg","","","1.34","1.34","1.34","1.34"]
["","Typ","","","","","","R-32","R-32","R-32","R-32"]
["Provozní rozsah","Chlazení","Okolí","Max.","°CST","","","43","43","43","43"]
["","","","Min.","°CST","","","-10","-10","-10","-10"]
["","Vytápění","Okolí","Max.","° CWB","","","18","18","18","18"]
["","","","Min.","° CWB","","","-20","-20","-20","-20"]
["Spoje potrubí","Rozdíl hladin","IU - OU","Max.","m","","","8","8","8","8"]
["Rozměry","Jednotka","","Šířka","mm","","","795","795","795","795"]
["","","","Hloubka","mm","","","300","300","300","300"]
["","","","Výška","mm","","","693","693","693","693"]
["Kompresor","Typ","","","","","","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor"]
["Hmotnost","Jednotka","","","kg","","","50","50","50","50"]
["Power supply","Fáze","","","","","","1~","1~","1~","1~"]
["","Frekvence","","","Hz","","","50","50","50","50"]
["","Napětí","","","V","","","220-240","220-240","220-240","220-240"]
["Poznámky","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V"]
["","","","","","","","(4) - Obsahuje fluorované skleníkové plyny","(4) - Obsahuje fluorované skleníkové plyny","(4) - Obsahuje fluorované skleníkové plyny","(4) - Obsahuje fluorované skleníkové plyny"]
["Rozměry","Jednotka","","Výška","mm","693","693"]
["","","","Šířka","mm","795","795"]
["","","","Hloubka","mm","300","300"]
["Hmotnost","Jednotka","","","kg","50","50"]
["Kompresor","Typ","","","","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor"]
["Provozní rozsah","Chlazení","Okolí","Min.","°CST","-10","-10"]
["","","","Max.","°CST","43","43"]
["","Vytápění","Okolí","Min.","° CWB","-20","-20"]
["","","","Max.","° CWB","18","18"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","46","46"]
["","Vytápění","","Vysoké","dBA","46","46"]
["Chladivo","Typ","","","","R-32","R-32"]
["","Náplň","","","kg","1.34","1.34"]
["","Náplň","","","tCO2Eq","0.9","0.9"]
["","Vliv na globální oteplování (GWP)","","","","675","675"]
["Spoje potrubí","Délka potrubí","Max.","OU - IU","m","10","10"]
["","Rozdíl hladin","IU - OU","Max.","m","8","8"]
["Standardní příslušenství","Installation manual","","","","1","1"]
["","Operation manual","","","","1","1"]
["Napájení","Fáze","","","","1~","1~"]
["","Frekvence","","","Hz","50","50"]
["","Napětí","","","V","220-240","220-240"]