{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZA-D"]
[]
[]
[]
[]
["","","","","","RZA200D7Y1B","RZA250D7Y1B"]
["Rozměry","Jednotka","","Výška","mm","870","870"]
["","","","Šířka","mm","1,100","1,100"]
["","","","Hloubka","mm","460","460"]
["Hmotnost","Jednotka","","","kg","117","117"]
["Kompresor","Typ","","","","Hermeticky utěsněný šroubový kompresor","Hermeticky utěsněný šroubový kompresor"]
["Provozní rozsah","Chlazení","Okolí","Min.","°CST","-20","-20"]
["","","","Max.","°CST","46","46"]
["","Vytápění","Okolí","Min.","° CWB","-20","-20"]
["","","","Max.","° CWB","15","15"]
["Sound power level","Chlazení","","","dBA","73","76"]
["","Vytápění","","","dBA","76 (1)","79 (1)"]
["Hladina akustického tlaku","Chlazení","","Jm.","dBA","53","57"]
["","Vytápění","","Jm.","dBA","60","63"]
["Chladivo","Typ","","","","R-32","R-32"]
["","Náplň","","","kg","5","5"]
["","Vliv na globální oteplování (GWP)","","","","675","675"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","9.52","9.52"]
["","Plyn","","Vnější průměr","mm","22.2","22.2"]
["","Délka potrubí","Max.","OU - IU","m","100","100"]
["","","Systém","Bez náplně","m","30","30"]
["","Doplňková náplň chladiva","","","kg/m","Viz instalační příručka","Viz instalační příručka"]
["Standardní příslušenství","Příručka pro instalaci","","","","1","1"]
["","Obecná bezpečnostní opatření","","","","1","1"]
["","Spojky pláště","","","","2","2"]
["","Odlepovací štítek pro F-plyny","","","","1","1"]
["","Propojovací potrubí","","","","6","6"]
["Power supply","Fáze","","","","3~","3~"]
["","Frekvence","","","Hz","50","50"]
["","Napětí","","","V","380-415","380-415"]
["Proud - 50 Hz","Max. proudová hodnota pojistky (MFA)","","","A","20","20"]
["Poznámky","","","","","(1) - V souladu s ENER Lot 21","(1) - V souladu s ENER Lot 21"]