{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":8,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-A"]
[]
[]
[]
[]
["","","","","","RZAG35A2V1B","RZAG50A2V1B","RZAG60A2V1B"]
["Rozměry","Jednotka","","Výška","mm","734","734","734"]
["","","","Šířka","mm","870","870","870"]
["","","","Hloubka","mm","373","373","373"]
["Hmotnost","Jednotka","","","kg","52","52","52"]
["Kompresor","Typ","","","","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor"]
["Hladina akustického výkonu","Chlazení","","","dBA","62.0","63.0","64.0"]
["","Vytápění","","","dBA","62.0","63.0","64.0"]
["Hladina akustického tlaku","Chlazení","","Jm.","dBA","48.0","49.0","50.0"]
["","Vytápění","","Jm.","dBA","48.0","49.0","50.0"]
["Chladivo","Typ","","","","","R-32"]
["","Náplň","","","kg","1.55","1.55","1.55"]
["","Vliv na globální oteplování (GWP)","","","","675.0","675.0","675.0"]
["","Náplň","","","tCO2Eq","1.05","1.05","1.05"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","6.35","6.35","6.35"]
["","Plyn","","Vnější průměr","mm","9.50","12.7","12.7"]
["Spoje potrubí","Délka potrubí","Max.","OU - IU","m","50","50","50"]
["","","Systém","Bez náplně","m","30","30","30"]
["","Doplňková náplň chladiva","","","kg/m","0,02 (pro délku potrubí přesahující 30m)","0,02 (pro délku potrubí přesahující 30m)","0,02 (pro délku potrubí přesahující 30m)"]
["","Rozdíl hladin","IU - OU","Max.","m","30.0","30.0","30.0"]
["Standardní příslušenství","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["Napájení","Fáze","","","","","1~"]
["","Frekvence","","","Hz","50","50","50"]
["","Napětí","","","V","","220-240"]