{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":7,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQ-C"]
[]
[]
[]
[]
["","","","","","RZQ200C7Y1B","RZQ250C7Y1B"]
["Rozměry","Jednotka","","Výška","mm","1,680"]
["","","","Šířka","mm","930"]
["","","","Hloubka","mm","765"]
["Hmotnost","Jednotka","","","kg","183.0"]
["Kompresor","Typ","","","","Hermeticky utěsněný šroubový kompresor"]
["Provozní rozsah","Chlazení","Okolí","Min.","°CDB","-5.0"]
["","","","Max.","°CDB","46.0"]
["","Vytápění","Okolí","Min.","° CWB","-15.0"]
["","","","Max.","° CWB","15.0"]
["Hladina akustického výkonu","Chlazení","","","dBA","78.0"]
["","Vytápění","","","dBA","78.0"]
["Chladivo","Typ","","","","R-410A"]
["","Náplň","","","kg","8.3"]
["","Vliv na globální oteplování (GWP)","","","","2,087.5"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","9.52"]
["","Plyn","","Vnější průměr","mm","22.2"]
["","Délka potrubí","Max.","OU - IU","m","100"]
["","","Systém","Bez náplně","m","30"]
["Standardní příslušenství","Příručka pro instalaci","","","","1"]
["","Propojovací potrubí","","","","4"]
["Power supply","Phase","","","","3N~"]
["","Frekvence","","","Hz","50"]
["","Napětí","","","V","380-415"]
["Proud - 50 Hz","Max. proudová hodnota pojistky (MFA)","","","A","25"]
["Poznámky","","","","","(1) - Napájení pro vnitřní jednotku FDQ je samostatné"]
["","","","","","(2) - Údaje o elektrickém systému najdete na zvláštním schématu"]
["Rozměry","Jednotka","","Výška","mm","","1680"]
["","","","Šířka","mm","","930"]
["","","","Hloubka","mm","","765"]
["Hmotnost","Jednotka","","","kg","","184.0"]
["Kompresor","Typ","","","","","Hermeticky utěsněný spirálový kompresor"]
["Provozní rozsah","Chlazení","Okolí","Min.","°CDB","","-5.0"]
["","","","Max.","°CDB","","46.0"]
["","Vytápění","Okolí","Min.","° CWB","","-15.0"]
["","","","Max.","° CWB","","15.0"]
["Hladina akustického výkonu","Chlazení","","","dBA","","78.0"]
["","Vytápění","","","dBA","","78.0"]
["Chladivo","Náplň","","","kg","","9.3"]
["","Vliv na globální oteplování (GWP)","","","","","2087.5"]
["","Náplň","","","tCO2Eq","","19.4"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","","12.70"]
["","Plyn","","Vnější průměr","mm","","22.2"]
["Spoje potrubí","Délka potrubí","Max.","OU - IU","m","","100"]
["","","Systém","Bez náplně","m","","30"]
["Standardní příslušenství","Installation manual","","","","","1"]
["","Connection pipes","","","","","4"]
["Napájení","Frekvence","","","Hz","","50"]
["Proud – 50&nbsp;Hz","Proud – 50&nbsp;Hz-=-Max. proudová hodnota pojistky (MFA)-=-A","","","A","","25"]